<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Capacitors - Aluminum Electrolytic Capacitors - WCAP-ATG5&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="https://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2022a, 2022-11-18&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-ATG5_8X14(DXL)">
<description>&lt;B&gt;WCAP-ATG5&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,8X14X3.5X0.5(DiameterXLengthXPitchXØPin)</description>
</package>
<package name="WCAP-ATG5_10X16(DXL)">
<description>&lt;B&gt;WCAP-ATG5&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X16X5X0.6(DiameterXLengthXPitchXØPin)</description>
</package>
<package name="WCAP-ATG5_18X45(DXL)">
<description>&lt;B&gt;WCAP-ATG5&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,18X45X7.5X0.8(DiameterXLengthXPitchXØPin)</description>
</package>
<package name="WCAP-ATG5_10X25(DXL)">
<description>&lt;B&gt;WCAP-ATG5&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X25X5X0.6(DiameterXLengthXPitchXØPin)</description>
</package>
<package name="WCAP-ATG5_8X16(DXL)">
<description>&lt;B&gt;WCAP-ATG5&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,8X16X3.5X0.5(DiameterXLengthXPitchXØPin)</description>
</package>
<package name="WCAP-ATG5_10X14(DXL)">
<description>&lt;B&gt;WCAP-ATG5&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X14X5X0.6(DiameterXLengthXPitchXØPin)</description>
</package>
<package name="WCAP-ATG5_10X12.5(DXL)">
<description>&lt;B&gt;WCAP-ATG5&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X12.5X5X0.6(DiameterXLengthXPitchXØPin)</description>
</package>
<package name="WCAP-ATG5_13X25(DXL)">
<description>&lt;B&gt;WCAP-ATG5&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,13X25X5X0.6(DiameterXLengthXPitchXØPin)</description>
</package>
<package name="WCAP-ATG5_18X31.5(DXL)">
<description>&lt;B&gt;WCAP-ATG5&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,18X31.5X7.5X0.8(DiameterXLengthXPitchXØPin)</description>
</package>
<package name="WCAP-ATG5_22X31(DXL)">
<description>&lt;B&gt;WCAP-ATG5&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,22X31X10X0.8(DiameterXLengthXPitchXØPin)</description>
</package>
<package name="WCAP-ATG5_5X11(DXL)">
<description>&lt;B&gt;WCAP-ATG5&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,5X11X2X0.5(DiameterXLengthXPitchXØPin)</description>
</package>
<package name="WCAP-ATG5_13X20(DXL)">
<description>&lt;B&gt;WCAP-ATG5&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,13X20X5X0.6(DiameterXLengthXPitchXØPin)</description>
</package>
<package name="WCAP-ATG5_10X20(DXL)">
<description>&lt;B&gt;WCAP-ATG5&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X20X5X0.6(DiameterXLengthXPitchXØPin)</description>
</package>
<package name="WCAP-ATG5_18X25(DXL)">
<description>&lt;B&gt;WCAP-ATG5&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,18X25X7.5X0.8(DiameterXLengthXPitchXØPin)</description>
</package>
<package name="WCAP-ATG5_25X51(DXL)">
<description>&lt;B&gt;WCAP-ATG5&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,25X51X12.5X1.0(DiameterXLengthXPitchXØPin)</description>
</package>
<package name="WCAP-ATG5_16X35.5(DXL)">
<description>&lt;B&gt;WCAP-ATG5&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,16X35.5X7.5X0.8(DiameterXLengthXPitchXØPin)</description>
</package>
<package name="WCAP-ATG5_16X31.5(DXL)">
<description>&lt;B&gt;WCAP-ATG5&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,16X31.5X7.5X0.8(DiameterXLengthXPitchXØPin)</description>
</package>
<package name="WCAP-ATG5_16X25(DXL)">
<description>&lt;B&gt;WCAP-ATG5&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,16X25X7.5X0.8(DiameterXLengthXPitchXØPin)</description>
</package>
<package name="WCAP-ATG5_8X11.5(DXL)">
<description>&lt;B&gt;WCAP-ATG5&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,8X11.5X3.5X0.5(DiameterXLengthXPitchXØPin)</description>
</package>
<package name="WCAP-ATG5_6.3X15(DXL)">
<description>&lt;B&gt;WCAP-ATG5&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,6.3X15X2.5X0.5(DiameterXLengthXPitchXØPin)</description>
</package>
<package name="WCAP-ATG5_18X35.5(DXL)">
<description>&lt;B&gt;WCAP-ATG5&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,18X35.5X7.5X0.8(DiameterXLengthXPitchXØPin)</description>
</package>
<package name="WCAP-ATG5_8X20(DXL)">
<description>&lt;B&gt;WCAP-ATG5&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,8X20X3.5X0.6(DiameterXLengthXPitchXØPin)</description>
</package>
<package name="WCAP-ATG5_6.3X11(DXL)">
<description>&lt;B&gt;WCAP-ATG5&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,6.3X11X2.5X0.5(DiameterXLengthXPitchXØPin)</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-ATG5_8X14" prefix="C">
<description>&lt;b&gt;WCAP-ATG5 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 18000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 31.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-ATG5&lt;/a&gt;&lt;p&gt;
Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG5_8X14(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860021374009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860021374009?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="81.6uA"/>
<attribute name="I-RIPPLE" value="75mA"/>
<attribute name="L" value="14mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860021374009 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJE1406R8M400DSPA7B000"/>
<attribute name="VALUE" value="6.8  uF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG5_18X45" prefix="C">
<description>&lt;b&gt;WCAP-ATG5 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 18000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 31.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-ATG5&lt;/a&gt;&lt;p&gt;
Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG5_18X45(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860021381024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860021381024?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="2160uA"/>
<attribute name="I-RIPPLE" value="700mA"/>
<attribute name="L" value="45mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860021381024 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJL450181M400DSPS1B000"/>
<attribute name="VALUE" value="180  uF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG5_10X16" prefix="C">
<description>&lt;b&gt;WCAP-ATG5 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 18000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 31.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-ATG5&lt;/a&gt;&lt;p&gt;
Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG5_10X16(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860020275016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020275016?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="120uA"/>
<attribute name="I-RIPPLE" value="630mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020275016 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF160122M010DSPAAB000"/>
<attribute name="VALUE" value="1200  uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860020275018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020275018?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="150uA"/>
<attribute name="I-RIPPLE" value="770mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020275018 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF160152M010DSPAAB000"/>
<attribute name="VALUE" value="1500  uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860020375016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020375016?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="131.2uA"/>
<attribute name="I-RIPPLE" value="550mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020375016 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF160821M016DSPAAB000"/>
<attribute name="VALUE" value="820  uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860020475015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020475015?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="140uA"/>
<attribute name="I-RIPPLE" value="460mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020475015 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF160561M025DSPAAB000"/>
<attribute name="VALUE" value="560  uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860020475016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020475016?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="170uA"/>
<attribute name="I-RIPPLE" value="520mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020475016 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF160681M025DSPAAB000"/>
<attribute name="VALUE" value="680  uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860020575014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020575014?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="164.5uA"/>
<attribute name="I-RIPPLE" value="520mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020575014 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF160471M035DSPAAB000"/>
<attribute name="VALUE" value="470  uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860020675021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020675021?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="165uA"/>
<attribute name="I-RIPPLE" value="450mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020675021 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF160331M050DSPAAB000"/>
<attribute name="VALUE" value="330  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860020775016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020775016?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="75.6uA"/>
<attribute name="I-RIPPLE" value="255mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020775016 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF160121M063DSPAAB000"/>
<attribute name="VALUE" value="120  uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860020775017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020775017?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="94.5uA"/>
<attribute name="I-RIPPLE" value="270mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020775017 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF160151M063DSPAAB000"/>
<attribute name="VALUE" value="150  uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860020775018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020775018?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="113.4uA"/>
<attribute name="I-RIPPLE" value="310mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020775018 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF160181M063DSPAAB000"/>
<attribute name="VALUE" value="180  uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860020775019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020775019?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="138.6uA"/>
<attribute name="I-RIPPLE" value="375mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020775019 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF160221M063DSPAAB000"/>
<attribute name="VALUE" value="220  uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG5_8X16" prefix="C">
<description>&lt;b&gt;WCAP-ATG5 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 18000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 31.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-ATG5&lt;/a&gt;&lt;p&gt;
Created by Ella Wu 2022-11-18
&lt;br&gt;2022(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG5_8X16(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860020374014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020374014?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="108.8uA"/>
<attribute name="I-RIPPLE" value="470mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020374014 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE160681M016DSPA7B000"/>
<attribute name="VALUE" value="680  uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860020674016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020674016?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="60uA"/>
<attribute name="I-RIPPLE" value="220mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020674016 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE160121M050DSPA7B000"/>
<attribute name="VALUE" value="120  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860021374027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860021374027?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="264uA"/>
<attribute name="I-RIPPLE" value="200mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860021374027"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJE1602203400DSPA7B0LR"/>
<attribute name="VALUE" value="22  uF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG5_10X25" prefix="C">
<description>&lt;b&gt;WCAP-ATG5 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 18000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 31.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-ATG5&lt;/a&gt;&lt;p&gt;
Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG5_10X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860021375012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860021375012?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="264uA"/>
<attribute name="I-RIPPLE" value="162mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860021375012 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJF250220M400DSPAAB000"/>
<attribute name="VALUE" value="22  uF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG5_10X14" prefix="C">
<description>&lt;b&gt;WCAP-ATG5 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 18000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 31.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-ATG5&lt;/a&gt;&lt;p&gt;
Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG5_10X14(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860021375011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860021375011?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="120uA"/>
<attribute name="I-RIPPLE" value="104mA"/>
<attribute name="L" value="14mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860021375011 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJF140100M400DSPA9B000"/>
<attribute name="VALUE" value="10  uF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG5_10X12.5" prefix="C">
<description>&lt;b&gt;WCAP-ATG5 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 18000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 31.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-ATG5&lt;/a&gt;&lt;p&gt;
Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG5_10X12.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860020275014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020275014?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="82uA"/>
<attribute name="I-RIPPLE" value="480mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020275014 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF125821M010DSPA9B000"/>
<attribute name="VALUE" value="820  uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860020275015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020275015?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="100uA"/>
<attribute name="I-RIPPLE" value="520mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020275015 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF125102M010DSPA9B000"/>
<attribute name="VALUE" value="1000  uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860020375013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020375013?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="89.6uA"/>
<attribute name="I-RIPPLE" value="410mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020375013 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF125561M016DSPA9B000"/>
<attribute name="VALUE" value="560  uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860020375015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020375015?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="108.8uA"/>
<attribute name="I-RIPPLE" value="480mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020375015 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF125681M016DSPA9B000"/>
<attribute name="VALUE" value="680  uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860020375017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020375017?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="160uA"/>
<attribute name="I-RIPPLE" value="540mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020375017 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF125102M016DSPA9B000"/>
<attribute name="VALUE" value="1000  uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860020575013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020575013?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="115.5uA"/>
<attribute name="I-RIPPLE" value="400mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020575013 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF125331M035DSPA9B000"/>
<attribute name="VALUE" value="330  uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860020675017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020675017?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="60uA"/>
<attribute name="I-RIPPLE" value="225mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020675017 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF125121M050DSPA9B000"/>
<attribute name="VALUE" value="120  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860020675018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020675018?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="75uA"/>
<attribute name="I-RIPPLE" value="245mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020675018 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF125151M050DSPA9B000"/>
<attribute name="VALUE" value="150  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860020675019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020675019?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="90uA"/>
<attribute name="I-RIPPLE" value="260mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020675019 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF125181M050DSPA9B000"/>
<attribute name="VALUE" value="180  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860020675020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020675020?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="110uA"/>
<attribute name="I-RIPPLE" value="345mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020675020 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF125221M050DSPA9B000"/>
<attribute name="VALUE" value="220  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860020775015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020775015?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="63uA"/>
<attribute name="I-RIPPLE" value="230mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020775015 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF125101M063DSPA9B000"/>
<attribute name="VALUE" value="100  uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860021375007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860021375007?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="39.6uA"/>
<attribute name="I-RIPPLE" value="41mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860021375007 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJF1253R3M400DSPA9B000"/>
<attribute name="VALUE" value="3.3  uF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
<technology name="_860021375010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860021375010?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="81.6uA"/>
<attribute name="I-RIPPLE" value="82mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860021375010 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJF1256R8M400DSPA9B000"/>
<attribute name="VALUE" value="6.8  uF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG5_13X25" prefix="C">
<description>&lt;b&gt;WCAP-ATG5 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 18000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 31.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-ATG5&lt;/a&gt;&lt;p&gt;
Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG5_13X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860020278025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020278025?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="470uA"/>
<attribute name="I-RIPPLE" value="1350mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020278025 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI250472M010DSPACB000"/>
<attribute name="VALUE" value="4700  uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860020378023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020378023?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="528uA"/>
<attribute name="I-RIPPLE" value="1200mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020378023 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI250332M016DSPACB000"/>
<attribute name="VALUE" value="3300  uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860020478021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020478021?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="450uA"/>
<attribute name="I-RIPPLE" value="1050mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020478021 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI250182M025DSPACB000"/>
<attribute name="VALUE" value="1800  uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860020478022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020478022?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="550uA"/>
<attribute name="I-RIPPLE" value="1200mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020478022 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI250222M025DSPACB000"/>
<attribute name="VALUE" value="2200  uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860020578020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020578020?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="525uA"/>
<attribute name="I-RIPPLE" value="960mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020578020 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI250152M035DSPACB000"/>
<attribute name="VALUE" value="1500  uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860020678025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020678025?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="410uA"/>
<attribute name="I-RIPPLE" value="850mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020678025 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI250821M050DSPACB000"/>
<attribute name="VALUE" value="820  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860020678026">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020678026?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="500uA"/>
<attribute name="I-RIPPLE" value="890mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020678026 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI250102M050DSPACB000"/>
<attribute name="VALUE" value="1000  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860020778022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020778022?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="352.8uA"/>
<attribute name="I-RIPPLE" value="770mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020778022 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI250561M063DSPACB000"/>
<attribute name="VALUE" value="560  uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG5_18X31.5" prefix="C">
<description>&lt;b&gt;WCAP-ATG5 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 18000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 31.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-ATG5&lt;/a&gt;&lt;p&gt;
Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG5_18X31.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860020581025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020581025?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1365uA"/>
<attribute name="I-RIPPLE" value="1820mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020581025 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDL315392M035DSPAEB000"/>
<attribute name="VALUE" value="3900  uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860020781027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020781027?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="945uA"/>
<attribute name="I-RIPPLE" value="1350mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020781027 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDL315152M063DSPAEB000"/>
<attribute name="VALUE" value="1500  uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860021381021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860021381021?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1440uA"/>
<attribute name="I-RIPPLE" value="550mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860021381021 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJL315121M400DSPAEB000"/>
<attribute name="VALUE" value="120  uF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG5_22X31" prefix="C">
<description>&lt;b&gt;WCAP-ATG5 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 18000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 31.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-ATG5&lt;/a&gt;&lt;p&gt;
Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG5_22X31(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860021383023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860021383023?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="1800uA"/>
<attribute name="I-RIPPLE" value="640mA"/>
<attribute name="L" value="31mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860021383023 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJN310151M400DSPS2B000"/>
<attribute name="VALUE" value="150  uF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG5_10X20" prefix="C">
<description>&lt;b&gt;WCAP-ATG5 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 18000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 31.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-ATG5&lt;/a&gt;&lt;p&gt;
Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG5_10X20(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860020275019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020275019?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="180uA"/>
<attribute name="I-RIPPLE" value="820mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020275019 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF200182M010DSPAAB000"/>
<attribute name="VALUE" value="1800  uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860020275020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020275020?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="220uA"/>
<attribute name="I-RIPPLE" value="860mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020275020 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF200222M010DSPAAB000"/>
<attribute name="VALUE" value="2200  uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860020375018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020375018?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="192uA"/>
<attribute name="I-RIPPLE" value="700mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020375018 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF200122M016DSPAAB000"/>
<attribute name="VALUE" value="1200  uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860020375019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020375019?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="240uA"/>
<attribute name="I-RIPPLE" value="820mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020375019 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF200152M016DSPAAB000"/>
<attribute name="VALUE" value="1500  uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860020475017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020475017?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="205uA"/>
<attribute name="I-RIPPLE" value="640mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020475017 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF200821M025DSPAAB000"/>
<attribute name="VALUE" value="820  uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860020475018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020475018?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="250uA"/>
<attribute name="I-RIPPLE" value="710mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020475018 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF200102M025DSPAAB000"/>
<attribute name="VALUE" value="1000  uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860020575015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020575015?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="196uA"/>
<attribute name="I-RIPPLE" value="540mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020575015 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF200561M035DSPAAB000"/>
<attribute name="VALUE" value="560  uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860020575016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020575016?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="238uA"/>
<attribute name="I-RIPPLE" value="560mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020575016 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF200681M035DSPAAB000"/>
<attribute name="VALUE" value="680  uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860020675022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020675022?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="235uA"/>
<attribute name="I-RIPPLE" value="600mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020675022 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF200471M050DSPAAB000"/>
<attribute name="VALUE" value="470  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG5_18X25" prefix="C">
<description>&lt;b&gt;WCAP-ATG5 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 18000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 31.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-ATG5&lt;/a&gt;&lt;p&gt;
Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG5_18X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860021381019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860021381019?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="984uA"/>
<attribute name="I-RIPPLE" value="470mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860021381019 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJL250820M400DSPAEB000"/>
<attribute name="VALUE" value="82  uF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG5_5X11" prefix="C">
<description>&lt;b&gt;WCAP-ATG5 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 18000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 31.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-ATG5&lt;/a&gt;&lt;p&gt;
Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG5_5X11(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860020272001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020272001?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="45mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020272001"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110220M010DSPA3B000"/>
<attribute name="VALUE" value="22  uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860020272002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020272002?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3.3uA"/>
<attribute name="I-RIPPLE" value="60mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020272002"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110330M010DSPA3B000"/>
<attribute name="VALUE" value="33  uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860020272003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020272003?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="4.7uA"/>
<attribute name="I-RIPPLE" value="70mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020272003"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110470M010DSPA3B000"/>
<attribute name="VALUE" value="47  uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860020272004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020272004?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="6.8uA"/>
<attribute name="I-RIPPLE" value="80mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020272004"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110680M010DSPA3B000"/>
<attribute name="VALUE" value="68  uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860020272005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020272005?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="105mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020272005"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110101M010DSPA3B000"/>
<attribute name="VALUE" value="100  uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860020272006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020272006?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="12uA"/>
<attribute name="I-RIPPLE" value="110mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020272006"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110121M010DSPA3B000"/>
<attribute name="VALUE" value="120  uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860020272007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020272007?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="15uA"/>
<attribute name="I-RIPPLE" value="120mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020272007"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110151M010DSPA3B000"/>
<attribute name="VALUE" value="150  uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860020372001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020372001?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="35mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020372001"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110100M016DSPA3B000"/>
<attribute name="VALUE" value="10  uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860020372002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020372002?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3.52uA"/>
<attribute name="I-RIPPLE" value="54mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020372002"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110220M016DSPA3B000"/>
<attribute name="VALUE" value="22  uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860020372003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020372003?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="5.28uA"/>
<attribute name="I-RIPPLE" value="64mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020372003"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110330M016DSPA3B000"/>
<attribute name="VALUE" value="33  uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860020372004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020372004?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="7.52uA"/>
<attribute name="I-RIPPLE" value="100mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020372004"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110470M016DSPA3B000"/>
<attribute name="VALUE" value="47  uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860020372005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020372005?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="10.88uA"/>
<attribute name="I-RIPPLE" value="105mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020372005"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110680M016DSPA3B000"/>
<attribute name="VALUE" value="68  uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860020372006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020372006?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="16uA"/>
<attribute name="I-RIPPLE" value="115mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020372006"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110101M016DSPA3B000"/>
<attribute name="VALUE" value="100  uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860020472001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020472001?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="26mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020472001"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC1104R7M025DSPA3B000"/>
<attribute name="VALUE" value="4.7  uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860020472002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020472002?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="32mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020472002"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC1106R8M025DSPA3B000"/>
<attribute name="VALUE" value="6.8  uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860020472003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020472003?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="38mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020472003"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110100M025DSPA3B000"/>
<attribute name="VALUE" value="10  uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860020472004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020472004?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="5.5uA"/>
<attribute name="I-RIPPLE" value="58mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020472004"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110220M025DSPA3B000"/>
<attribute name="VALUE" value="22  uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860020472005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020472005?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="8.25uA"/>
<attribute name="I-RIPPLE" value="69mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020472005"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110330M025DSPA3B000"/>
<attribute name="VALUE" value="33  uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860020472006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020472006?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="11.75uA"/>
<attribute name="I-RIPPLE" value="105mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020472006"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110470M025DSPA3B000"/>
<attribute name="VALUE" value="47  uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860020572001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020572001?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="28mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020572001"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC1104R7M035DSPA3B000"/>
<attribute name="VALUE" value="4.7  uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860020572002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020572002?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="36mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020572002"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC1106R8M035DSPA3B000"/>
<attribute name="VALUE" value="6.8  uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860020572003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020572003?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3.5uA"/>
<attribute name="I-RIPPLE" value="46mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020572003"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110100M035DSPA3B000"/>
<attribute name="VALUE" value="10  uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860020572004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020572004?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="7.7uA"/>
<attribute name="I-RIPPLE" value="61mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020572004"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110220M035DSPA3B000"/>
<attribute name="VALUE" value="22  uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860020572005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020572005?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="11.55uA"/>
<attribute name="I-RIPPLE" value="75mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020572005"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110330M035DSPA3B000"/>
<attribute name="VALUE" value="33  uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860020572006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020572006?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="16.45uA"/>
<attribute name="I-RIPPLE" value="110mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020572006"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110470M035DSPA3B000"/>
<attribute name="VALUE" value="47  uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860020672001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020672001?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="1.3mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020672001"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110R10M050DSPA3B000"/>
<attribute name="VALUE" value="0.1  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860020672002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020672002?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="2.9mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020672002"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110R22M050DSPA3B000"/>
<attribute name="VALUE" value="0.22  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860020672003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020672003?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="4mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020672003"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110R33M050DSPA3B000"/>
<attribute name="VALUE" value="0.33  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860020672004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020672004?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="7mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020672004"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110R47M050DSPA3B000"/>
<attribute name="VALUE" value="0.47  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860020672005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020672005?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="13mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020672005"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110010M050DSPA3B000"/>
<attribute name="VALUE" value="1  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860020672006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020672006?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="20mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020672006"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC1102R2M050DSPA3B000"/>
<attribute name="VALUE" value="2.2  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860020672007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020672007?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="26mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020672007"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC1103R3M050DSPA3B000"/>
<attribute name="VALUE" value="3.3  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860020672008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020672008?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="32mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020672008"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC1104R7M050DSPA3B000"/>
<attribute name="VALUE" value="4.7  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860020672009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020672009?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3.4uA"/>
<attribute name="I-RIPPLE" value="40mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020672009"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC1106R8M050DSPA3B000"/>
<attribute name="VALUE" value="6.8  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860020672010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020672010?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="5uA"/>
<attribute name="I-RIPPLE" value="48mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020672010"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110100M050DSPA3B000"/>
<attribute name="VALUE" value="10  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860020672011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020672011?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="11uA"/>
<attribute name="I-RIPPLE" value="60mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020672011"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110220M050DSPA3B000"/>
<attribute name="VALUE" value="22  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860020672012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020672012?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="16.5uA"/>
<attribute name="I-RIPPLE" value="75mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020672012"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110330M050DSPA3B000"/>
<attribute name="VALUE" value="33  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860020772001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020772001?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="1.3mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020772001"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110R10M063DSPA3B000"/>
<attribute name="VALUE" value="0.1  uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860020772002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020772002?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="2.9mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020772002"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110R22M063DSPA3B000"/>
<attribute name="VALUE" value="0.22  uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860020772003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020772003?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="4.5mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020772003"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110R33M063DSPA3B000"/>
<attribute name="VALUE" value="0.33  uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860020772004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020772004?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="7mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020772004"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110R47M063DSPA3B000"/>
<attribute name="VALUE" value="0.47  uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860020772005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020772005?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="13mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020772005"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110010M063DSPA3B000"/>
<attribute name="VALUE" value="1  uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860020772006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020772006?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="20mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020772006"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC1102R2M063DSPA3B000"/>
<attribute name="VALUE" value="2.2  uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860020772007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020772007?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="28mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020772007"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC1103R3M063DSPA3B000"/>
<attribute name="VALUE" value="3.3  uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860020772008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020772008?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="32mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020772008"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC1104R7M063DSPA3B000"/>
<attribute name="VALUE" value="4.7  uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860020772009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020772009?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="4.284uA"/>
<attribute name="I-RIPPLE" value="40mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020772009"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC1106R8M063DSPA3B000"/>
<attribute name="VALUE" value="6.8  uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860020772010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020772010?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="6.3uA"/>
<attribute name="I-RIPPLE" value="42mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020772010"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110100M063DSPA3B000"/>
<attribute name="VALUE" value="10  uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG5_13X20" prefix="C">
<description>&lt;b&gt;WCAP-ATG5 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 18000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 31.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-ATG5&lt;/a&gt;&lt;p&gt;
Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG5_13X20(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860020275021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020275021?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="270uA"/>
<attribute name="I-RIPPLE" value="880mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020275021 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF250272M010DSPAAB000"/>
<attribute name="VALUE" value="2700  uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860020278022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020278022?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="270uA"/>
<attribute name="I-RIPPLE" value="920mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020278022 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI200272M010DSPACB000"/>
<attribute name="VALUE" value="2700  uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860020278023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020278023?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="330uA"/>
<attribute name="I-RIPPLE" value="1100mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020278023 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI200332M010DSPACB000"/>
<attribute name="VALUE" value="3300  uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860020278024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020278024?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="390uA"/>
<attribute name="I-RIPPLE" value="1280mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020278024 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI200392M010DSPACB000"/>
<attribute name="VALUE" value="3900  uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860020378020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020378020?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="288uA"/>
<attribute name="I-RIPPLE" value="920mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020378020 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI200182M016DSPACB000"/>
<attribute name="VALUE" value="1800  uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860020378021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020378021?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="352uA"/>
<attribute name="I-RIPPLE" value="1000mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020378021 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI200222M016DSPACB000"/>
<attribute name="VALUE" value="2200  uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860020378022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020378022?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="432uA"/>
<attribute name="I-RIPPLE" value="1080mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020378022 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI200272M016DSPACB000"/>
<attribute name="VALUE" value="2700  uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860020478019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020478019?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="300uA"/>
<attribute name="I-RIPPLE" value="810mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020478019 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI200122M025DSPACB000"/>
<attribute name="VALUE" value="1200  uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860020478020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020478020?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="375uA"/>
<attribute name="I-RIPPLE" value="900mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020478020 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI200152M025DSPACB000"/>
<attribute name="VALUE" value="1500  uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860020578017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020578017?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="287uA"/>
<attribute name="I-RIPPLE" value="760mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020578017 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI200821M035DSPACB000"/>
<attribute name="VALUE" value="820  uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860020578018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020578018?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="350uA"/>
<attribute name="I-RIPPLE" value="830mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020578018 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI200102M035DSPACB000"/>
<attribute name="VALUE" value="1000  uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860020578019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020578019?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="420uA"/>
<attribute name="I-RIPPLE" value="900mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020578019 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI200122M035DSPACB000"/>
<attribute name="VALUE" value="1200  uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860020678023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020678023?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="280uA"/>
<attribute name="I-RIPPLE" value="660mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020678023 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI200561M050DSPACB000"/>
<attribute name="VALUE" value="560  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860020678024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020678024?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="340uA"/>
<attribute name="I-RIPPLE" value="700mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020678024 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI200681M050DSPACB000"/>
<attribute name="VALUE" value="680  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860020778020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020778020?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="207.9uA"/>
<attribute name="I-RIPPLE" value="580mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020778020 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI200331M063DSPACB000"/>
<attribute name="VALUE" value="330  uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860020778021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020778021?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="296.1uA"/>
<attribute name="I-RIPPLE" value="690mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020778021 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI200471M063DSPACB000"/>
<attribute name="VALUE" value="470  uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860021378013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860021378013?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="264uA"/>
<attribute name="I-RIPPLE" value="170mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860021378013 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJI200220M400DSPACB000"/>
<attribute name="VALUE" value="22  uF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
<technology name="_860021378014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860021378014?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="396uA"/>
<attribute name="I-RIPPLE" value="235mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860021378014 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJI200330M400DSPACB000"/>
<attribute name="VALUE" value="33  uF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG5_16X35.5" prefix="C">
<description>&lt;b&gt;WCAP-ATG5 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 18000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 31.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-ATG5&lt;/a&gt;&lt;p&gt;
Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG5_16X35.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860020280029">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020280029?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="1000uA"/>
<attribute name="I-RIPPLE" value="1900mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020280029 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK355103M010DSPADB000"/>
<attribute name="VALUE" value="10000  uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860020280030">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020280030?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="1200uA"/>
<attribute name="I-RIPPLE" value="2050mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020280030 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK355123M010DSPADB000"/>
<attribute name="VALUE" value="12000  uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860020380028">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020380028?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="1312uA"/>
<attribute name="I-RIPPLE" value="2020mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020380028 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK355822M016DSPADB000"/>
<attribute name="VALUE" value="8200  uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860020480026">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020480026?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="1175uA"/>
<attribute name="I-RIPPLE" value="1780mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020480026 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK355472M025DSPADB000"/>
<attribute name="VALUE" value="4700  uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860020480027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020480027?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="1400uA"/>
<attribute name="I-RIPPLE" value="1890mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020480027 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK355562M025DSPADB000"/>
<attribute name="VALUE" value="5600  uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860020580024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020580024?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="1155uA"/>
<attribute name="I-RIPPLE" value="1650mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020580024 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK355332M035DSPADB000"/>
<attribute name="VALUE" value="3300  uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860020680029">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020680029?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="900uA"/>
<attribute name="I-RIPPLE" value="1480mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020680029 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK355182M050DSPADB000"/>
<attribute name="VALUE" value="1800  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860020680030">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020680030?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="1100uA"/>
<attribute name="I-RIPPLE" value="1530mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020680030 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK355222M050DSPADB000"/>
<attribute name="VALUE" value="2200  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860020780026">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020780026?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="756uA"/>
<attribute name="I-RIPPLE" value="1200mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020780026 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK355122M063DSPADB000"/>
<attribute name="VALUE" value="1200  uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG5_16X25" prefix="C">
<description>&lt;b&gt;WCAP-ATG5 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 18000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 31.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-ATG5&lt;/a&gt;&lt;p&gt;
Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG5_16X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860020280026">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020280026?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="560uA"/>
<attribute name="I-RIPPLE" value="1490mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020280026 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK250562M010DSPAEB000"/>
<attribute name="VALUE" value="5600  uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860020280027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020280027?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="680uA"/>
<attribute name="I-RIPPLE" value="1670mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020280027 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK250682M010DSPAEB000"/>
<attribute name="VALUE" value="6800  uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860020380024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020380024?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="624uA"/>
<attribute name="I-RIPPLE" value="1490mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020380024 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK250392M016DSPAEB000"/>
<attribute name="VALUE" value="3900  uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860020380025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020380025?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="752uA"/>
<attribute name="I-RIPPLE" value="1600mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020380025 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK250472M016DSPAEB000"/>
<attribute name="VALUE" value="4700  uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860020480023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020480023?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="675uA"/>
<attribute name="I-RIPPLE" value="1320mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020480023 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK250272M025DSPAEB000"/>
<attribute name="VALUE" value="2700  uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860020480024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020480024?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="825uA"/>
<attribute name="I-RIPPLE" value="1460mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020480024 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK250332M025DSPAEB000"/>
<attribute name="VALUE" value="3300  uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860020580021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020580021?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="630uA"/>
<attribute name="I-RIPPLE" value="1150mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020580021 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK250182M035DSPAEB000"/>
<attribute name="VALUE" value="1800  uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860020580022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020580022?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="770uA"/>
<attribute name="I-RIPPLE" value="1290mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020580022 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK250222M035DSPAEB000"/>
<attribute name="VALUE" value="2200  uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860020680027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020680027?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="1150mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020680027 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK250122M050DSPAEB000"/>
<attribute name="VALUE" value="1200  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860020780023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020780023?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="428.4uA"/>
<attribute name="I-RIPPLE" value="880mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020780023 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK250681M063DSPAEB000"/>
<attribute name="VALUE" value="680  uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860020780024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020780024?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="516.6uA"/>
<attribute name="I-RIPPLE" value="920mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020780024 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK250821M063DSPAEB000"/>
<attribute name="VALUE" value="820  uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860021380015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860021380015?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="564uA"/>
<attribute name="I-RIPPLE" value="300mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860021380015 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJK250470M400DSPAEB000"/>
<attribute name="VALUE" value="47  uF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
<technology name="_860021380016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860021380016?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="672uA"/>
<attribute name="I-RIPPLE" value="360mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860021380016 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJK250560M400DSPAEB000"/>
<attribute name="VALUE" value="56  uF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
<technology name="_860021380017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860021380017?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="816uA"/>
<attribute name="I-RIPPLE" value="410mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860021380017 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJK250680M400DSPAEB000"/>
<attribute name="VALUE" value="68  uF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG5_16X31.5" prefix="C">
<description>&lt;b&gt;WCAP-ATG5 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 18000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 31.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-ATG5&lt;/a&gt;&lt;p&gt;
Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG5_16X31.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860020280028">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020280028?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="820uA"/>
<attribute name="I-RIPPLE" value="1840mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020280028 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK315822M010DSPADB000"/>
<attribute name="VALUE" value="8200  uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860020380026">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020380026?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="896uA"/>
<attribute name="I-RIPPLE" value="1720mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020380026 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK315562M016DSPADB000"/>
<attribute name="VALUE" value="5600  uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860020380027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020380027?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="1088uA"/>
<attribute name="I-RIPPLE" value="1900mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020380027 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK315682M016DSPADB000"/>
<attribute name="VALUE" value="6800  uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860020480025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020480025?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="975uA"/>
<attribute name="I-RIPPLE" value="1670mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020480025 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK315392M025DSPADB000"/>
<attribute name="VALUE" value="3900  uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860020580023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020580023?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="945uA"/>
<attribute name="I-RIPPLE" value="1480mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020580023 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK315272M035DSPADB000"/>
<attribute name="VALUE" value="2700  uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860020680028">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020680028?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="750uA"/>
<attribute name="I-RIPPLE" value="1300mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020680028 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK315152M050DSPADB000"/>
<attribute name="VALUE" value="1500  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860020780025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020780025?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="630uA"/>
<attribute name="I-RIPPLE" value="1185mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020780025 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK315102M063DSPADB000"/>
<attribute name="VALUE" value="1000  uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860021380018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860021380018?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="984uA"/>
<attribute name="I-RIPPLE" value="480mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860021380018 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJK315820M400DSPADB000"/>
<attribute name="VALUE" value="82  uF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
<technology name="_860021380020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860021380020?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="1200uA"/>
<attribute name="I-RIPPLE" value="520mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860021380020 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJK315101M400DSPADB000"/>
<attribute name="VALUE" value="100  uF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG5_8X11.5" prefix="C">
<description>&lt;b&gt;WCAP-ATG5 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 18000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 31.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-ATG5&lt;/a&gt;&lt;p&gt;
Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG5_8X11.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860020274012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020274012?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="56uA"/>
<attribute name="I-RIPPLE" value="330mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020274012 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE115561M010DSPA7B000"/>
<attribute name="VALUE" value="560  uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860020274013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020274013?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="68uA"/>
<attribute name="I-RIPPLE" value="365mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020274013 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE115681M010DSPA7B000"/>
<attribute name="VALUE" value="680  uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860020374012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020374012?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="75.2uA"/>
<attribute name="I-RIPPLE" value="370mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020374012 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE115471M016DSPA7B000"/>
<attribute name="VALUE" value="470  uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860020474011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020474011?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="45uA"/>
<attribute name="I-RIPPLE" value="210mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020474011 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE115181M025DSPA7B000"/>
<attribute name="VALUE" value="180  uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860020474012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020474012?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="55uA"/>
<attribute name="I-RIPPLE" value="235mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020474012 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE115221M025DSPA7B000"/>
<attribute name="VALUE" value="220  uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860020474013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020474013?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="82.5uA"/>
<attribute name="I-RIPPLE" value="310mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020474013 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE115331M025DSPA7B000"/>
<attribute name="VALUE" value="330  uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860020474014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020474014?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="117.5uA"/>
<attribute name="I-RIPPLE" value="410mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020474014 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE115471M025DSPA7B000"/>
<attribute name="VALUE" value="470  uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860020574009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020574009?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="42uA"/>
<attribute name="I-RIPPLE" value="185mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020574009 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE115121M035DSPA7B000"/>
<attribute name="VALUE" value="120  uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860020574010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020574010?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="52.5uA"/>
<attribute name="I-RIPPLE" value="215mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020574010 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE115151M035DSPA7B000"/>
<attribute name="VALUE" value="150  uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860020574011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020574011?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="63uA"/>
<attribute name="I-RIPPLE" value="225mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020574011 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE115181M035DSPA7B000"/>
<attribute name="VALUE" value="180  uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860020574012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020574012?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="77uA"/>
<attribute name="I-RIPPLE" value="255mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020574012 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE115221M035DSPA7B000"/>
<attribute name="VALUE" value="220  uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860020674015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020674015?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="50uA"/>
<attribute name="I-RIPPLE" value="200mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020674015 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE115101M050DSPA7B000"/>
<attribute name="VALUE" value="100  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860020774014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020774014?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="42.84uA"/>
<attribute name="I-RIPPLE" value="155mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020774014 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE115680M063DSPA7B000"/>
<attribute name="VALUE" value="68  uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860021374004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860021374004?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="26.4uA"/>
<attribute name="I-RIPPLE" value="35mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860021374004 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJE1152R2M400DSPA7B000"/>
<attribute name="VALUE" value="2.2  uF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
<technology name="_860021374006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860021374006?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="39.6uA"/>
<attribute name="I-RIPPLE" value="36mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860021374006 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJE1153R3M400DSPA7B000"/>
<attribute name="VALUE" value="3.3  uF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
<technology name="_860021374008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860021374008?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="56.4uA"/>
<attribute name="I-RIPPLE" value="48mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860021374008 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJE1154R7M400DSPA7B000"/>
<attribute name="VALUE" value="4.7  uF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG5_6.3X15" prefix="C">
<description>&lt;b&gt;WCAP-ATG5 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 18000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 31.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-ATG5&lt;/a&gt;&lt;p&gt;
Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG5_6.3X15(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860021373003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860021373003?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="26.4uA"/>
<attribute name="I-RIPPLE" value="34mA"/>
<attribute name="L" value="15mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860021373003 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJD1502R2M400DSPA4B000"/>
<attribute name="VALUE" value="2.2  uF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
<technology name="_860021373005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860021373005?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="39.6uA"/>
<attribute name="I-RIPPLE" value="35mA"/>
<attribute name="L" value="15mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860021373005 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJD1503R3M400DSPA4B000"/>
<attribute name="VALUE" value="3.3  uF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
<technology name="_860021373025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860021373025?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="56.4uA"/>
<attribute name="I-RIPPLE" value="50mA"/>
<attribute name="L" value="15mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860021373025 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJD1504R7M400DSPA4B000"/>
<attribute name="VALUE" value="4.7  uF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG5_25X51" prefix="C">
<description>&lt;b&gt;WCAP-ATG5 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 18000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 31.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-ATG5&lt;/a&gt;&lt;p&gt;
Created by Ella Wu 2022-11-18
&lt;br&gt;2022(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG5_25X51(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860020684033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020684033?ae"/>
<attribute name="DF" value="28%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="5000uA"/>
<attribute name="I-RIPPLE" value="3600mA"/>
<attribute name="L" value="51mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020684033"/>
<attribute name="PITCH" value="12.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDO510103M050DSPS2B000"/>
<attribute name="VALUE" value="50  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG5_18X35.5" prefix="C">
<description>&lt;b&gt;WCAP-ATG5 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 18000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 31.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-ATG5&lt;/a&gt;&lt;p&gt;
Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG5_18X35.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860020281031">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020281031?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1500uA"/>
<attribute name="I-RIPPLE" value="2180mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020281031 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDL355153M010DSPAEB000"/>
<attribute name="VALUE" value="15000  uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860020281032">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020281032?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1800uA"/>
<attribute name="I-RIPPLE" value="2205mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020281032 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDL355183M010DSPAEB000"/>
<attribute name="VALUE" value="18000  uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860020381029">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020381029?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1600uA"/>
<attribute name="I-RIPPLE" value="2060mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020381029 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDL355103M016DSPAEB000"/>
<attribute name="VALUE" value="10000  uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860020381030">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020381030?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1920uA"/>
<attribute name="I-RIPPLE" value="2150mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020381030 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDL355123M016DSPAEB000"/>
<attribute name="VALUE" value="12000  uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860020481028">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020481028?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1700uA"/>
<attribute name="I-RIPPLE" value="2050mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020481028 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDL355682M025DSPAEB000"/>
<attribute name="VALUE" value="6800  uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860020481029">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020481029?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="2050uA"/>
<attribute name="I-RIPPLE" value="2090mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020481029 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDL355822M025DSPAEB000"/>
<attribute name="VALUE" value="8200  uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860020581026">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020581026?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1645uA"/>
<attribute name="I-RIPPLE" value="1900mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020581026 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDL355472M035DSPAEB000"/>
<attribute name="VALUE" value="4700  uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860020581027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020581027?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1960uA"/>
<attribute name="I-RIPPLE" value="2000mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020581027 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDL355562M035DSPAEB000"/>
<attribute name="VALUE" value="5600  uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860020681031">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020681031?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1350uA"/>
<attribute name="I-RIPPLE" value="1590mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020681031 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDL355272M050DSPAEB000"/>
<attribute name="VALUE" value="2700  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860020681032">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020681032?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1650uA"/>
<attribute name="I-RIPPLE" value="1750mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020681032 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDL355332M050DSPAEB000"/>
<attribute name="VALUE" value="3300  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860021381022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860021381022?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1800uA"/>
<attribute name="I-RIPPLE" value="610mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860021381022 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJL355151M400DSPAEB000"/>
<attribute name="VALUE" value="150  uF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG5_6.3X11" prefix="C">
<description>&lt;b&gt;WCAP-ATG5 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 18000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 31.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-ATG5&lt;/a&gt;&lt;p&gt;
Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG5_6.3X11(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860020273008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020273008?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="18uA"/>
<attribute name="I-RIPPLE" value="160mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020273008 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110181M010DSPA4B000"/>
<attribute name="VALUE" value="180  uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860020273009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020273009?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="22uA"/>
<attribute name="I-RIPPLE" value="175mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020273009 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110221M010DSPA4B000"/>
<attribute name="VALUE" value="220  uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860020273010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020273010?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="33uA"/>
<attribute name="I-RIPPLE" value="205mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020273010 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110331M010DSPA4B000"/>
<attribute name="VALUE" value="330  uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860020273011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020273011?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="47uA"/>
<attribute name="I-RIPPLE" value="235mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020273011 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110471M010DSPA4B000"/>
<attribute name="VALUE" value="470  uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860020373007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020373007?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="19.2uA"/>
<attribute name="I-RIPPLE" value="155mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020373007"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110121M016DSPA4B000"/>
<attribute name="VALUE" value="120  uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860020373008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020373008?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="24uA"/>
<attribute name="I-RIPPLE" value="170mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020373008"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110151M016DSPA4B000"/>
<attribute name="VALUE" value="150  uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860020373009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020373009?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="28.8uA"/>
<attribute name="I-RIPPLE" value="190mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860020373009"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110181M016DSPA4B000"/>
<attribute name="VALUE" value="180  uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860020373010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020373010?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="35.2uA"/>
<attribute name="I-RIPPLE" value="215mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020373010 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110221M016DSPA4B000"/>
<attribute name="VALUE" value="220  uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860020373011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020373011?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="52.8uA"/>
<attribute name="I-RIPPLE" value="225mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020373011 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110331M016DSPA4B000"/>
<attribute name="VALUE" value="330  uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860020473007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020473007?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="17uA"/>
<attribute name="I-RIPPLE" value="120mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020473007 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110680M025DSPA4B000"/>
<attribute name="VALUE" value="68  uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860020473008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020473008?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="25uA"/>
<attribute name="I-RIPPLE" value="145mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020473008 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110101M025DSPA4B000"/>
<attribute name="VALUE" value="100  uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860020473009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020473009?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="30uA"/>
<attribute name="I-RIPPLE" value="175mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020473009 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110121M025DSPA4B000"/>
<attribute name="VALUE" value="120  uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860020473010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020473010?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="37.5uA"/>
<attribute name="I-RIPPLE" value="180mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020473010 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110151M025DSPA4B000"/>
<attribute name="VALUE" value="150  uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860020573007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020573007?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="23.8uA"/>
<attribute name="I-RIPPLE" value="140mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020573007 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110680M035DSPA4B000"/>
<attribute name="VALUE" value="68  uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860020573008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020573008?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="35uA"/>
<attribute name="I-RIPPLE" value="160mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020573008 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110101M035DSPA4B000"/>
<attribute name="VALUE" value="100  uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860020673013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020673013?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="23.5uA"/>
<attribute name="I-RIPPLE" value="115mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020673013 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110470M050DSPA4B000"/>
<attribute name="VALUE" value="47  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860020673014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020673014?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="34uA"/>
<attribute name="I-RIPPLE" value="130mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020673014 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110680M050DSPA4B000"/>
<attribute name="VALUE" value="68  uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860020773011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020773011?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="13.86uA"/>
<attribute name="I-RIPPLE" value="82mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020773011 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110220M063DSPA4B000"/>
<attribute name="VALUE" value="22  uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860020773012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020773012?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="20.79uA"/>
<attribute name="I-RIPPLE" value="100mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020773012 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110330M063DSPA4B000"/>
<attribute name="VALUE" value="33  uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860020773013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020773013?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="29.61uA"/>
<attribute name="I-RIPPLE" value="125mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020773013 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110470M063DSPA4B000"/>
<attribute name="VALUE" value="47  uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860021373001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860021373001?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="5.64uA"/>
<attribute name="I-RIPPLE" value="14mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860021373001 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJD110R47M400DSPA4B000"/>
<attribute name="VALUE" value="0.47  uF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
<technology name="_860021373002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860021373002?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="12uA"/>
<attribute name="I-RIPPLE" value="17mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860021373002 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJD110010M400DSPA4B000"/>
<attribute name="VALUE" value="1  uF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG5_8X20" prefix="C">
<description>&lt;b&gt;WCAP-ATG5 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 18000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 31.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o683503v209%20family-wcap-atg5-860020672004.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ATG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-ATG5&lt;/a&gt;&lt;p&gt;
Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG5_8X20(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860020274017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860020274017?ae"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="150uA"/>
<attribute name="I-RIPPLE" value="715mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860020274017 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE200152M010DSPA7B000"/>
<attribute name="VALUE" value="1500  uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>