<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Quartz Crystals &amp; Oscillators - WE-XTAL&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="https://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-03-10&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-XTAL_HC49/4H">
<description>&lt;b&gt;WE-XTAL Quartz Crystal
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;HC49/4H, THT, 2pins
&lt;br&gt;L X W X H = 11.05mm X 4.7mm X 4.1mm</description>
</package>
<package name="WE-XTAL_HC49/4HSMX">
<description>&lt;b&gt;WE-XTAL Quartz Crystal
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;HC49/4HSMX, SMT, 2pins
&lt;br&gt;L X W X H = 11.3mm X 4.7mm X 4.5mm</description>
</package>
<package name="WE-XTAL_CFPX-180">
<description>&lt;b&gt;WE-XTAL Quartz Crystal
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;CFPX-180, SMT, 4pins
&lt;br&gt;L X W X H = 3.4mm X 2.7mm X 0.8mm</description>
</package>
<package name="WE-XTAL_IQXC-25">
<description>&lt;b&gt;WE-XTAL Quartz Crystal
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;IQXC-25, SMT, 4pins 
&lt;br&gt;L X W X H = 2mm X 1mm X 0.6mm</description>
</package>
<package name="WE-XTAL_IQXC-146">
<description>&lt;b&gt;WE-XTAL Quartz Crystal
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;IQXC-146, SMT, 4pins
&lt;br&gt;L X W X H = 1.27mm X 1.05mm X 0.5mm</description>
</package>
<package name="WE-XTAL_CFPX-56">
<description>&lt;b&gt;WE-XTAL Watch Crystals
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;CFPX-56， SMT, 2pins
&lt;br&gt;L X W X H = 6mm X 1.8mm X 1.8mm</description>
</package>
<package name="WE-XTAL_IQXC-26">
<description>&lt;b&gt;WE-XTAL Quartz Crystal
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;IQXC-26, SMT, 4pins
&lt;br&gt;L X W X H = 1.6mm X 1.2mm X 0.4mm</description>
</package>
<package name="WE-XTAL_HC49">
<description>&lt;b&gt;WE-XTAL Quartz Crystal
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;HC49, THT, 2pins
&lt;br&gt;L X W X H = 11.05mm X 10.2mm X 13.46mm</description>
</package>
<package name="WE-XTAL_WATCH-3X8">
<description>&lt;b&gt;WE-XTAL Quartz Crystal
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;WATCH_2X8, THT, 2pins
&lt;br&gt;Body Diameter X H = 3mm  X 8.2mm</description>
</package>
<package name="WE-XTAL_CFPX-218">
<description>&lt;b&gt;WE-XTAL Quartz Crystal
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;CFPX-218, SMT, 4pins
&lt;br&gt;L X W X H = 2.5mm X 2mm X 0.6mm</description>
</package>
<package name="WE-XTAL_WATCH-2X6">
<description>&lt;b&gt;WE-XTAL Quartz Crystal
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;WATCH_2X6, THT, 2pins
&lt;br&gt;Body Diameter X H = 2mm  X 6.2mm</description>
</package>
<package name="WE-XTAL_IQXC-42">
<description>&lt;b&gt;WE-XTAL Quartz Crystal
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;IQXC-42, SMT, 4pins
&lt;br&gt;L X W X H = 2mm X 1.6mm X 0.5mm</description>
</package>
<package name="WE-XTAL_IQXC-90">
<description>&lt;b&gt;WE-XTAL Watch Crystals
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;IQXC-90, SMT, 2pins
&lt;br&gt;L X W X H = 1.6mm X 1mm X 0.5mm</description>
</package>
<package name="WE-XTAL_IQXC-240">
<description>&lt;b&gt;WE-XTAL Watch Crystals 
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;IQXC-240, SMT, 4pins
&lt;br&gt;L X W X H = 1.2mm X 1.0mm X 0.5mm</description>
</package>
<package name="WE-XTAL_CFPX-104">
<description>&lt;b&gt;WE-XTAL Quartz Crystal
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;CFPX-104, SMT, 4pins
&lt;br&gt;L X W X H = 5mm X 3.2mm X 1mm</description>
</package>
<package name="WE-XTAL_85SMX">
<description>&lt;b&gt;WE-XTAL Watch Crystals
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;85SMX, SMT, 4pins
&lt;br&gt;L X W X H = 8.7mm X 3.8mm X 2.5mm</description>
</package>
<package name="WE-XTAL_CFPX-217">
<description>&lt;b&gt;WE-XTAL Watch Crystals
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;CFPX-217, SMT, 2pins
&lt;br&gt;L X W X H = 3.2mm X 1.5mm X 0.9mm</description>
</package>
<package name="WE-XTAL_12SMX">
<description>&lt;b&gt;WE-XTAL Quartz Crystal
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;12SMX, SMT, 4pins
&lt;br&gt;L X W X H = 7.0mm X 5.0mm X 1.2mm</description>
</package>
</packages>
<symbols>
<symbol name="CRYSTAL">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="CRYSTAL-4PIN">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND1" direction="pas"/>
</symbol>
<symbol name="CRYSTAL-4PIN_NC">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="N/C" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-XTAL_HC49/4H" prefix="Y">
<description>&lt;b&gt;WE-XTAL Quartz Crystal
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;SMT and THT models
&lt;br&gt; Hermetically sealed
&lt;br&gt; Frequencies between 1.8432 MHz and 50 MHz
&lt;br&gt; Tolerances down to ±10 ppm available
&lt;br&gt; Maximum operating temperatures range: -40 °C to 85 °C
&lt;br&gt; Stabilities down to ±10 ppm available
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;&lt;br&gt;
&lt;br&gt; Microprocessor
&lt;br&gt; Wireless Communication Devices
&lt;br&gt; Industrial Devices
&lt;br&gt; Wired Communication (e.g. Ethernet and USB)
&lt;br&gt; IoT
&lt;br&gt; Optical Network
&lt;br&gt; Audio and Multimedia Devices
&lt;br&gt; Test and Measurement Equipment
&lt;br&gt; Navigation and Locators
&lt;br&gt; Wearables
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135919v209%20WE%20XTAL%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135919v209%20WE%20XTAL%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XTAL&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-10&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CRYSTAL"/>
</gates>
<devices>
<device name="" package="WE-XTAL_HC49/4H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_830003063B">
<attribute name="C-LOAD" value="20pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003063B?ae"/>
<attribute name="FREQUENCY" value="3.579545 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830003063B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="3.579545 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830003074B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003074B?ae"/>
<attribute name="FREQUENCY" value="4 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003074B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="4 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830003084B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003084B?ae"/>
<attribute name="FREQUENCY" value="4.096 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003084B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="4.096 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830003093B">
<attribute name="C-LOAD" value="12pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003093B?ae"/>
<attribute name="FREQUENCY" value="4.194304 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003093B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="4.194304 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830003102B">
<attribute name="C-LOAD" value="20pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003102B?ae"/>
<attribute name="FREQUENCY" value="4.433619 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003102B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="4.433619 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830003115B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003115B?ae"/>
<attribute name="FREQUENCY" value="4.9152 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830003115B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="4.9152 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830003119B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003119B?ae"/>
<attribute name="FREQUENCY" value="5 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003119B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="5 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830003132B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003132B?ae"/>
<attribute name="FREQUENCY" value="6 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003132B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="6 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830003137B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003137B?ae"/>
<attribute name="FREQUENCY" value="6.144 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003137B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="6.144 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830003156B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003156B?ae"/>
<attribute name="FREQUENCY" value="8 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830003156B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="8 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830003169B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003169B?ae"/>
<attribute name="FREQUENCY" value="10 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830003169B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="10 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830003176B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003176B?ae"/>
<attribute name="FREQUENCY" value="18.432 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830003176B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="18.432 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830003185B">
<attribute name="C-LOAD" value="12pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003185B?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830003185B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830003186B">
<attribute name="C-LOAD" value="20pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003186B?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003186B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830003200B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003200B?ae"/>
<attribute name="FREQUENCY" value="14.31818 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830003200B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="14.31818 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830003215B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003215B?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830003215B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830003224B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003224B?ae"/>
<attribute name="FREQUENCY" value="14.7456 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003224B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="14.7456 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830003240B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003240B?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830003240B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830003263B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003263B?ae"/>
<attribute name="FREQUENCY" value="3.6864 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830003263B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="3.6864 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830003271B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003271B?ae"/>
<attribute name="FREQUENCY" value="8.192 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003271B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="8.192 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830003279B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003279B?ae"/>
<attribute name="FREQUENCY" value="9.8304 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003279B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="9.8304 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830003286B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003286B?ae"/>
<attribute name="FREQUENCY" value="12.288 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003286B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="12.288 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830003309B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003309B?ae"/>
<attribute name="FREQUENCY" value="19.6608 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003309B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="19.6608 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830003325B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003325B?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003325B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830003335B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003335B?ae"/>
<attribute name="FREQUENCY" value="7.3728 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003335B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="7.3728 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830003336B">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003336B?ae"/>
<attribute name="FREQUENCY" value="7.3728 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003336B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±15ppm"/>
<attribute name="VALUE" value="7.3728 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830003523B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003523B?ae"/>
<attribute name="FREQUENCY" value="11.0592 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830003523B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="11.0592 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830014948B">
<attribute name="C-LOAD" value="pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830014948B?ae"/>
<attribute name="FREQUENCY" value="27.12 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830014948B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="27.12 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830018496B">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830018496B?ae"/>
<attribute name="FREQUENCY" value="11.0592 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830018496B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="11.0592 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830024985B">
<attribute name="C-LOAD" value="12pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830024985B?ae"/>
<attribute name="FREQUENCY" value="3.2768 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830024985B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="3.2768 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830027298B">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830027298B?ae"/>
<attribute name="FREQUENCY" value="4 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830027298B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="4 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830031646B">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830031646B?ae"/>
<attribute name="FREQUENCY" value="13 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830031646B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="13 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830032341B">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830032341B?ae"/>
<attribute name="FREQUENCY" value="10 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830032341B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="10 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
<technology name="_830058383B">
<attribute name="C-LOAD" value="20pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830058383B?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="LENGTH" value="11.35mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830058383B"/>
<attribute name="SIZE" value="HC49/4H"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="4.85mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XTAL_HC49/4HSMX" prefix="Y">
<description>&lt;b&gt;WE-XTAL Quartz Crystal
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;SMT and THT models
&lt;br&gt; Hermetically sealed
&lt;br&gt; Frequencies between 1.8432 MHz and 50 MHz
&lt;br&gt; Tolerances down to ±10 ppm available
&lt;br&gt; Maximum operating temperatures range: -40 °C to 85 °C
&lt;br&gt; Stabilities down to ±10 ppm available
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;&lt;br&gt;
&lt;br&gt; Microprocessor
&lt;br&gt; Wireless Communication Devices
&lt;br&gt; Industrial Devices
&lt;br&gt; Wired Communication (e.g. Ethernet and USB)
&lt;br&gt; IoT
&lt;br&gt; Optical Network
&lt;br&gt; Audio and Multimedia Devices
&lt;br&gt; Test and Measurement Equipment
&lt;br&gt; Navigation and Locators
&lt;br&gt; Wearables
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135919v209%20WE%20XTAL%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135919v209%20WE%20XTAL%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XTAL&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-10&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CRYSTAL"/>
</gates>
<devices>
<device name="" package="WE-XTAL_HC49/4HSMX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_830003058">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003058?ae"/>
<attribute name="FREQUENCY" value="3.579545 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003058"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="3.579545 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003071">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003071?ae"/>
<attribute name="FREQUENCY" value="4 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003071"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="4 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003151">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003151?ae"/>
<attribute name="FREQUENCY" value="8 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003151"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="8 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003166">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003166?ae"/>
<attribute name="FREQUENCY" value="10 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003166"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="10 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003181">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003181?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003181"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003210">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003210?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003210"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003237">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003237?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003237"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003260">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003260?ae"/>
<attribute name="FREQUENCY" value="3.6864 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003260"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="3.6864 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003334">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003334?ae"/>
<attribute name="FREQUENCY" value="7.3728 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003334"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="7.3728 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003387">
<attribute name="C-LOAD" value="20pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003387?ae"/>
<attribute name="FREQUENCY" value="24.576 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003387"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="24.576 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003519">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003519?ae"/>
<attribute name="FREQUENCY" value="11.0592 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003519"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="11.0592 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830010043">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830010043?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830010043"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830010595">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830010595?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830010595"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830010689">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830010689?ae"/>
<attribute name="FREQUENCY" value="7.3728 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830010689"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="7.3728 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830011263">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830011263?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830011263"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830011300">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830011300?ae"/>
<attribute name="FREQUENCY" value="4 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830011300"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="4 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830011301">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830011301?ae"/>
<attribute name="FREQUENCY" value="8 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830011301"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="8 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830012312">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830012312?ae"/>
<attribute name="FREQUENCY" value="5 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830012312"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="5 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830012313">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830012313?ae"/>
<attribute name="FREQUENCY" value="14.7456 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830012313"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="14.7456 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830012504">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830012504?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830012504"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830015023">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830015023?ae"/>
<attribute name="FREQUENCY" value="18.432 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830015023"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="18.432 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830015055">
<attribute name="C-LOAD" value="20pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830015055?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830015055"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830016788">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830016788?ae"/>
<attribute name="FREQUENCY" value="6 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830016788"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="6 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830017145">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830017145?ae"/>
<attribute name="FREQUENCY" value="10 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830017145"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="10 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830017146">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830017146?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830017146"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830018153">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830018153?ae"/>
<attribute name="FREQUENCY" value="4.9152 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830018153"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="4.9152 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830020131">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830020131?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830020131"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830020423">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830020423?ae"/>
<attribute name="FREQUENCY" value="8 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830020423"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="8 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830021675">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830021675?ae"/>
<attribute name="FREQUENCY" value="10 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830021675"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="10 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830024940">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830024940?ae"/>
<attribute name="FREQUENCY" value="4 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830024940"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="4 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830026548">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830026548?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830026548"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830026900">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830026900?ae"/>
<attribute name="FREQUENCY" value="6 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830026900"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="6 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830026902">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830026902?ae"/>
<attribute name="FREQUENCY" value="8.192 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830026902"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="8.192 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830026904">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830026904?ae"/>
<attribute name="FREQUENCY" value="9.8304 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830026904"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="9.8304 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830026908">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830026908?ae"/>
<attribute name="FREQUENCY" value="14.7456 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830026908"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="14.7456 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830026911">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830026911?ae"/>
<attribute name="FREQUENCY" value="18.432 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830026911"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="18.432 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830027527">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830027527?ae"/>
<attribute name="FREQUENCY" value="7.175 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="830027527"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="100ppm"/>
<attribute name="TOLERANCE" value="±50ppm"/>
<attribute name="VALUE" value="7.175 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830028392">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830028392?ae"/>
<attribute name="FREQUENCY" value="4.9152 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830028392"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="4.9152 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830028430">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830028430?ae"/>
<attribute name="FREQUENCY" value="3.2768 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830028430"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="3.2768 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830028710">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830028710?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830028710"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830028928">
<attribute name="C-LOAD" value="20pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830028928?ae"/>
<attribute name="FREQUENCY" value="11.0592 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830028928"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="11.0592 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830029370">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830029370?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830029370"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830029914">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830029914?ae"/>
<attribute name="FREQUENCY" value="8 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830029914"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="8 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830030798">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830030798?ae"/>
<attribute name="FREQUENCY" value="3.6864 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830030798"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="3.6864 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830033158">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830033158?ae"/>
<attribute name="FREQUENCY" value="3.6864 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830033158"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="3.6864 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830033580">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830033580?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830033580"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830034122">
<attribute name="C-LOAD" value="12pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830034122?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830034122"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830034225">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830034225?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-30 °C up to +80 °C"/>
<attribute name="PART-NUMBER" value="830034225"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±50ppm"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830034439">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830034439?ae"/>
<attribute name="FREQUENCY" value="4.9152 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830034439"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="4.9152 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830034654">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830034654?ae"/>
<attribute name="FREQUENCY" value="4 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830034654"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="4 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830035293">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830035293?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830035293"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830036034">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830036034?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830036034"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830036533">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830036533?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830036533"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830036956">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830036956?ae"/>
<attribute name="FREQUENCY" value="14.7456 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830036956"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="14.7456 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830050510">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830050510?ae"/>
<attribute name="FREQUENCY" value="8 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830050510"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="8 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830051235">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830051235?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830051235"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830054555">
<attribute name="C-LOAD" value="20pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830054555?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830054555"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830056463">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830056463?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830056463"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830061856">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830061856?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830061856"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="10ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830063075">
<attribute name="C-LOAD" value="22pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830063075?ae"/>
<attribute name="FREQUENCY" value="17.2032 MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830063075"/>
<attribute name="SIZE" value="HC49/4HSMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="17.2032 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XTAL_CFPX-180" prefix="Y">
<description>&lt;b&gt;WE-XTAL Quartz Crystal
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;SMT and THT models
&lt;br&gt; Hermetically sealed
&lt;br&gt; Frequencies between 1.8432 MHz and 50 MHz
&lt;br&gt; Tolerances down to ±10 ppm available
&lt;br&gt; Maximum operating temperatures range: -40 °C to 85 °C
&lt;br&gt; Stabilities down to ±10 ppm available
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;&lt;br&gt;
&lt;br&gt; Microprocessor
&lt;br&gt; Wireless Communication Devices
&lt;br&gt; Industrial Devices
&lt;br&gt; Wired Communication (e.g. Ethernet and USB)
&lt;br&gt; IoT
&lt;br&gt; Optical Network
&lt;br&gt; Audio and Multimedia Devices
&lt;br&gt; Test and Measurement Equipment
&lt;br&gt; Navigation and Locators
&lt;br&gt; Wearables
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135919v209%20WE%20XTAL%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135919v209%20WE%20XTAL%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XTAL&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-10&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CRYSTAL-4PIN"/>
</gates>
<devices>
<device name="" package="WE-XTAL_CFPX-180">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="GND" pad="2" route="any"/>
<connect gate="G$1" pin="GND1" pad="4"/>
</connects>
<technologies>
<technology name="_830035264">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830035264?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830035264"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±50ppm"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830035265">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830035265?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830035265"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±50ppm"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830035266">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830035266?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830035266"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±50ppm"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830035267">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830035267?ae"/>
<attribute name="FREQUENCY" value="24.576 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830035267"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±50ppm"/>
<attribute name="VALUE" value="24.576 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830035268">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830035268?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830035268"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±50ppm"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830035269">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830035269?ae"/>
<attribute name="FREQUENCY" value="30 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830035269"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±50ppm"/>
<attribute name="VALUE" value="30 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830035503">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830035503?ae"/>
<attribute name="FREQUENCY" value="16.384 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830035503"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±50ppm"/>
<attribute name="VALUE" value="16.384 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830051068">
<attribute name="C-LOAD" value="9pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830051068?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830051068"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="10ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830053099">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830053099?ae"/>
<attribute name="FREQUENCY" value="27.12 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830053099"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="10ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="27.12 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830055293">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830055293?ae"/>
<attribute name="FREQUENCY" value="14.7456 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830055293"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="14.7456 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830055295">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830055295?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830055295"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830055299">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830055299?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830055299"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830055474">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830055474?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830055474"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±50ppm"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830055951">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830055951?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830055951"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830055962">
<attribute name="C-LOAD" value="12pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830055962?ae"/>
<attribute name="FREQUENCY" value="30 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830055962"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="10ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="30 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830056346">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830056346?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830056346"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830057824">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830057824?ae"/>
<attribute name="FREQUENCY" value="27 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830057824"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="27 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830058124">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830058124?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830058124"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830058149">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830058149?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830058149"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="10ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830059638">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830059638?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830059638"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830059643">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830059643?ae"/>
<attribute name="FREQUENCY" value="26 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830059643"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="26 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830059646">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830059646?ae"/>
<attribute name="FREQUENCY" value="30 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830059646"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="30 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830059648">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830059648?ae"/>
<attribute name="FREQUENCY" value="40 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830059648"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="40 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830059800">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830059800?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830059800"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="10ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830060258">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830060258?ae"/>
<attribute name="FREQUENCY" value="32 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830060258"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="32 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830060843">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830060843?ae"/>
<attribute name="FREQUENCY" value="50 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830060843"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="TOLERANCE" value="±25ppm"/>
<attribute name="VALUE" value="50 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830061647">
<attribute name="C-LOAD" value="12pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830061647?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830061647"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830061648">
<attribute name="C-LOAD" value="12pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830061648?ae"/>
<attribute name="FREQUENCY" value="12.288 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830061648"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="12.288 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830061677">
<attribute name="C-LOAD" value="12pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830061677?ae"/>
<attribute name="FREQUENCY" value="32 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830061677"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="32 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830063321">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830063321?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830063321"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830064296">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830064296?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830064296"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830064703">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830064703?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830064703"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830068911">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830068911?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830068911"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830069377">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830069377?ae"/>
<attribute name="FREQUENCY" value="32 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830069377"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="32 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830069882">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830069882?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="830069882"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="100ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830069944">
<attribute name="C-LOAD" value="15pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830069944?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830069944"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830070868">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830070868?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830070868"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830072604">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830072604?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830072604"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830082070">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830082070?ae"/>
<attribute name="FREQUENCY" value="13.56 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830082070"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="13.56 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830100965009">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830100965009?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830100965009"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830103552209">
<attribute name="C-LOAD" value="9pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830103552209?ae"/>
<attribute name="FREQUENCY" value="32 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830103552209"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="32 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830103622909">
<attribute name="C-LOAD" value="9pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830103622909?ae"/>
<attribute name="FREQUENCY" value="32 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830103622909"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="15ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="32 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830105420809">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830105420809?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830105420809"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="10ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830105863709">
<attribute name="C-LOAD" value="12pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830105863709?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830105863709"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830105957509">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830105957509?ae"/>
<attribute name="FREQUENCY" value="24.576 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830105957509"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="24.576 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830105961109">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830105961109?ae"/>
<attribute name="FREQUENCY" value="13.56 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830105961109"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="13.56 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830105961309">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830105961309?ae"/>
<attribute name="FREQUENCY" value="14.31818 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830105961309"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="14.31818 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830105961509">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830105961509?ae"/>
<attribute name="FREQUENCY" value="16.384 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830105961509"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="16.384 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830105961709">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830105961709?ae"/>
<attribute name="FREQUENCY" value="18.432 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830105961709"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="18.432 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830106246109">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830106246109?ae"/>
<attribute name="FREQUENCY" value="27.12 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830106246109"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="27.12 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830107006509">
<attribute name="C-LOAD" value="9pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830107006509?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830107006509"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="15ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830107878109">
<attribute name="C-LOAD" value="12pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830107878109?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="830107878109"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830108174209">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108174209?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108174209"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="15ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830108206909">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108206909?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108206909"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830108207109">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108207109?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108207109"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830108207209">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108207209?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108207209"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830108207309">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108207309?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108207309"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830108207409">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108207409?ae"/>
<attribute name="FREQUENCY" value="27 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108207409"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="27 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830108207509">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108207509?ae"/>
<attribute name="FREQUENCY" value="30 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108207509"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="30 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830108207609">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108207609?ae"/>
<attribute name="FREQUENCY" value="32 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108207609"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="32 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830108207709">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108207709?ae"/>
<attribute name="FREQUENCY" value="40 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108207709"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="40 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830108207809">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108207809?ae"/>
<attribute name="FREQUENCY" value="50 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108207809"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="50 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830108313809">
<attribute name="C-LOAD" value="12pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108313809?ae"/>
<attribute name="FREQUENCY" value="8 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108313809"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="8 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830108338709">
<attribute name="C-LOAD" value="12pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108338709?ae"/>
<attribute name="FREQUENCY" value="10 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="830108338709"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="10 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830108338809">
<attribute name="C-LOAD" value="12pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108338809?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="830108338809"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830108340709">
<attribute name="C-LOAD" value="12pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108340709?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="830108340709"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830108340809">
<attribute name="C-LOAD" value="12pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108340809?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="830108340809"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830108340909">
<attribute name="C-LOAD" value="12pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108340909?ae"/>
<attribute name="FREQUENCY" value="26 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="830108340909"/>
<attribute name="SIZE" value="CFPX-180"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="26 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XTAL_IQXC-25" prefix="Y">
<description>&lt;b&gt;WE-XTAL Watch Crystals
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;SMT and THT models
&lt;br&gt;Hermetically sealed
&lt;br&gt;Frequency: 32.768 kHz
&lt;br&gt;Tolerances down to ±10 ppm available
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Microprocessor
&lt;br&gt;Real Time Clocks
&lt;br&gt;Test and Measurement Equipment
&lt;br&gt;Battery powered Applications
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o162740v209%20WE%20Watch%20XTAL%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o162740v209%20WE%20Watch%20XTAL%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XTAL_WATCHCRYSTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XTAL_WATCHCRYSTAL&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CRYSTAL"/>
</gates>
<devices>
<device name="" package="WE-XTAL_IQXC-25">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_830050789">
<attribute name="C-LOAD" value="12.5pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830050789?ae"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830050789"/>
<attribute name="SIZE" value="IQXC-25"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="32.768 kHz"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_830062558">
<attribute name="C-LOAD" value="9pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830062558?ae"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830062558"/>
<attribute name="SIZE" value="IQXC-25"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="32.768 kHz"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_830105946101">
<attribute name="C-LOAD" value="7pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830105946101?ae"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830105946101"/>
<attribute name="SIZE" value="IQXC-25"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="32.768 kHz"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_830106545501">
<attribute name="C-LOAD" value="6pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830106545501?ae"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830106545501"/>
<attribute name="SIZE" value="IQXC-25"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="32.768 kHz"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_830107326401">
<attribute name="C-LOAD" value="4pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830107326401?ae"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830107326401"/>
<attribute name="SIZE" value="IQXC-25"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="32.768 kHz"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XTAL_CFPX-56" prefix="Y">
<description>&lt;b&gt;WE-XTAL Watch Crystals
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;SMT and THT models
&lt;br&gt;Hermetically sealed
&lt;br&gt;Frequency: 32.768 kHz
&lt;br&gt;Tolerances down to ±10 ppm available
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Microprocessor
&lt;br&gt;Real Time Clocks
&lt;br&gt;Test and Measurement Equipment
&lt;br&gt;Battery powered Applications
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o162740v209%20WE%20Watch%20XTAL%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o162740v209%20WE%20Watch%20XTAL%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XTAL_WATCHCRYSTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XTAL_WATCHCRYSTAL&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CRYSTAL"/>
</gates>
<devices>
<device name="" package="WE-XTAL_CFPX-56">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_830025159">
<attribute name="C-LOAD" value="12.5pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830025159?ae"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="2.54mm"/>
<attribute name="LENGTH" value="9.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830025159"/>
<attribute name="SIZE" value="CFPX-56"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="32.768 kHz"/>
<attribute name="WIDTH" value="2.54mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XTAL_IQXC-26" prefix="Y">
<description>&lt;b&gt;WE-XTAL Quartz Crystal
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;SMT and THT models
&lt;br&gt; Hermetically sealed
&lt;br&gt; Frequencies between 1.8432 MHz and 50 MHz
&lt;br&gt; Tolerances down to ±10 ppm available
&lt;br&gt; Maximum operating temperatures range: -40 °C to 85 °C
&lt;br&gt; Stabilities down to ±10 ppm available
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;&lt;br&gt;
&lt;br&gt; Microprocessor
&lt;br&gt; Wireless Communication Devices
&lt;br&gt; Industrial Devices
&lt;br&gt; Wired Communication (e.g. Ethernet and USB)
&lt;br&gt; IoT
&lt;br&gt; Optical Network
&lt;br&gt; Audio and Multimedia Devices
&lt;br&gt; Test and Measurement Equipment
&lt;br&gt; Navigation and Locators
&lt;br&gt; Wearables
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135919v209%20WE%20XTAL%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135919v209%20WE%20XTAL%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XTAL&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-10&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CRYSTAL-4PIN"/>
</gates>
<devices>
<device name="" package="WE-XTAL_IQXC-26">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="GND" pad="2" route="any"/>
<connect gate="G$1" pin="GND1" pad="4"/>
</connects>
<technologies>
<technology name="_830066742">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830066742?ae"/>
<attribute name="FREQUENCY" value="26 MHz"/>
<attribute name="HEIGHT" value="0.4mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830066742"/>
<attribute name="SIZE" value="IQXC-26"/>
<attribute name="STABILITY" value="15ppm"/>
<attribute name="TOLERANCE" value="±15ppm"/>
<attribute name="VALUE" value="26 MHz"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_830069526">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830069526?ae"/>
<attribute name="FREQUENCY" value="32 MHz"/>
<attribute name="HEIGHT" value="0.4mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830069526"/>
<attribute name="SIZE" value="IQXC-26"/>
<attribute name="STABILITY" value="15ppm"/>
<attribute name="TOLERANCE" value="±15ppm"/>
<attribute name="VALUE" value="32 MHz"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_830069527">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830069527?ae"/>
<attribute name="FREQUENCY" value="40 MHz"/>
<attribute name="HEIGHT" value="0.4mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830069527"/>
<attribute name="SIZE" value="IQXC-26"/>
<attribute name="STABILITY" value="15ppm"/>
<attribute name="TOLERANCE" value="±15ppm"/>
<attribute name="VALUE" value="40 MHz"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_830069528">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830069528?ae"/>
<attribute name="FREQUENCY" value="48 MHz"/>
<attribute name="HEIGHT" value="0.4mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830069528"/>
<attribute name="SIZE" value="IQXC-26"/>
<attribute name="STABILITY" value="15ppm"/>
<attribute name="TOLERANCE" value="±15ppm"/>
<attribute name="VALUE" value="48 MHz"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_830072539">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830072539?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="0.4mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830072539"/>
<attribute name="SIZE" value="IQXC-26"/>
<attribute name="STABILITY" value="15ppm"/>
<attribute name="TOLERANCE" value="±15ppm"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_830072541">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830072541?ae"/>
<attribute name="FREQUENCY" value="27 MHz"/>
<attribute name="HEIGHT" value="0.4mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830072541"/>
<attribute name="SIZE" value="IQXC-26"/>
<attribute name="STABILITY" value="15ppm"/>
<attribute name="TOLERANCE" value="±15ppm"/>
<attribute name="VALUE" value="27 MHz"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_830081609">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830081609?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="0.4mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830081609"/>
<attribute name="SIZE" value="IQXC-26"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_830081620">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830081620?ae"/>
<attribute name="FREQUENCY" value="48 MHz"/>
<attribute name="HEIGHT" value="0.4mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830081620"/>
<attribute name="SIZE" value="IQXC-26"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="48 MHz"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_830108160801">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108160801?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="0.4mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108160801"/>
<attribute name="SIZE" value="IQXC-26"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_830108161001">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108161001?ae"/>
<attribute name="FREQUENCY" value="27 MHz"/>
<attribute name="HEIGHT" value="0.4mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108161001"/>
<attribute name="SIZE" value="IQXC-26"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="27 MHz"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_830108161201">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108161201?ae"/>
<attribute name="FREQUENCY" value="30 MHz"/>
<attribute name="HEIGHT" value="0.4mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108161201"/>
<attribute name="SIZE" value="IQXC-26"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="30 MHz"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_830108161301">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108161301?ae"/>
<attribute name="FREQUENCY" value="32 MHz"/>
<attribute name="HEIGHT" value="0.4mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108161301"/>
<attribute name="SIZE" value="IQXC-26"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="32 MHz"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_830108161401">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108161401?ae"/>
<attribute name="FREQUENCY" value="26 MHz"/>
<attribute name="HEIGHT" value="0.4mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108161401"/>
<attribute name="SIZE" value="IQXC-26"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="26 MHz"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_830108161601">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108161601?ae"/>
<attribute name="FREQUENCY" value="37.4 MHz"/>
<attribute name="HEIGHT" value="0.4mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108161601"/>
<attribute name="SIZE" value="IQXC-26"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="37.4 MHz"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_830108161901">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108161901?ae"/>
<attribute name="FREQUENCY" value="40 MHz"/>
<attribute name="HEIGHT" value="0.4mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108161901"/>
<attribute name="SIZE" value="IQXC-26"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="40 MHz"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XTAL_IQXC-146" prefix="Y">
<description>&lt;b&gt;WE-XTAL Watch Crystals
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;SMT and THT models
&lt;br&gt;Hermetically sealed
&lt;br&gt;Frequency: 32.768 kHz
&lt;br&gt;Tolerances down to ±10 ppm available
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Microprocessor
&lt;br&gt;Real Time Clocks
&lt;br&gt;Test and Measurement Equipment
&lt;br&gt;Battery powered Applications
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o162740v209%20WE%20Watch%20XTAL%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o162740v209%20WE%20Watch%20XTAL%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XTAL_WATCHCRYSTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XTAL_WATCHCRYSTAL&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CRYSTAL-4PIN_NC"/>
</gates>
<devices>
<device name="" package="WE-XTAL_IQXC-146">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="N/C" pad="4"/>
</connects>
<technologies>
<technology name="_830107834801">
<attribute name="C-LOAD" value="6pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830107834801?ae"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830107834801"/>
<attribute name="SIZE" value="IQXC-146"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="32.768 kHz"/>
<attribute name="WIDTH" value="1mm"/>
</technology>
<technology name="_830108091501">
<attribute name="C-LOAD" value="12.5pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108091501?ae"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108091501"/>
<attribute name="SIZE" value="IQXC-146"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="32.768 kHz"/>
<attribute name="WIDTH" value="1mm"/>
</technology>
<technology name="_830108211801">
<attribute name="C-LOAD" value="7pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108211801?ae"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108211801"/>
<attribute name="SIZE" value="IQXC-146"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="32.768 kHz"/>
<attribute name="WIDTH" value="1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XTAL_HC49" prefix="Y">
<description>&lt;b&gt;WE-XTAL Quartz Crystal
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;SMT and THT models
&lt;br&gt; Hermetically sealed
&lt;br&gt; Frequencies between 1.8432 MHz and 50 MHz
&lt;br&gt; Tolerances down to ±10 ppm available
&lt;br&gt; Maximum operating temperatures range: -40 °C to 85 °C
&lt;br&gt; Stabilities down to ±10 ppm available
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;&lt;br&gt;
&lt;br&gt; Microprocessor
&lt;br&gt; Wireless Communication Devices
&lt;br&gt; Industrial Devices
&lt;br&gt; Wired Communication (e.g. Ethernet and USB)
&lt;br&gt; IoT
&lt;br&gt; Optical Network
&lt;br&gt; Audio and Multimedia Devices
&lt;br&gt; Test and Measurement Equipment
&lt;br&gt; Navigation and Locators
&lt;br&gt; Wearables
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135919v209%20WE%20XTAL%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135919v209%20WE%20XTAL%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XTAL&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-10&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CRYSTAL"/>
</gates>
<devices>
<device name="" package="WE-XTAL_HC49">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_830003033B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003033B?ae"/>
<attribute name="FREQUENCY" value="1.8432 MHz"/>
<attribute name="HEIGHT" value="13.49mm"/>
<attribute name="LENGTH" value="11.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003033B"/>
<attribute name="SIZE" value="HC49"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="1.8432 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003037B">
<attribute name="C-LOAD" value="20pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003037B?ae"/>
<attribute name="FREQUENCY" value="2 MHz"/>
<attribute name="HEIGHT" value="13.49mm"/>
<attribute name="LENGTH" value="11.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +50 °C"/>
<attribute name="PART-NUMBER" value="830003037B"/>
<attribute name="SIZE" value="HC49"/>
<attribute name="STABILITY" value="100ppm"/>
<attribute name="TOLERANCE" value="±50ppm"/>
<attribute name="VALUE" value="2 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003044B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003044B?ae"/>
<attribute name="FREQUENCY" value="2.4576 MHz"/>
<attribute name="HEIGHT" value="13.49mm"/>
<attribute name="LENGTH" value="11.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003044B"/>
<attribute name="SIZE" value="HC49"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="2.4576 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003051B">
<attribute name="C-LOAD" value="12pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003051B?ae"/>
<attribute name="FREQUENCY" value="3.2768 MHz"/>
<attribute name="HEIGHT" value="13.49mm"/>
<attribute name="LENGTH" value="11.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003051B"/>
<attribute name="SIZE" value="HC49"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="3.2768 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003056B">
<attribute name="C-LOAD" value="20pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003056B?ae"/>
<attribute name="FREQUENCY" value="3.579545 MHz"/>
<attribute name="HEIGHT" value="13.49mm"/>
<attribute name="LENGTH" value="11.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003056B"/>
<attribute name="SIZE" value="HC49"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="3.579545 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003068B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003068B?ae"/>
<attribute name="FREQUENCY" value="4 MHz"/>
<attribute name="HEIGHT" value="13.49mm"/>
<attribute name="LENGTH" value="11.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003068B"/>
<attribute name="SIZE" value="HC49"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="4 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003086B">
<attribute name="C-LOAD" value="12pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003086B?ae"/>
<attribute name="FREQUENCY" value="4.194304 MHz"/>
<attribute name="HEIGHT" value="13.49mm"/>
<attribute name="LENGTH" value="11.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003086B"/>
<attribute name="SIZE" value="HC49"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="4.194304 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003099B">
<attribute name="C-LOAD" value="20pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003099B?ae"/>
<attribute name="FREQUENCY" value="4.433619 MHz"/>
<attribute name="HEIGHT" value="13.49mm"/>
<attribute name="LENGTH" value="11.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003099B"/>
<attribute name="SIZE" value="HC49"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="4.433619 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003110B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003110B?ae"/>
<attribute name="FREQUENCY" value="4.9152 MHz"/>
<attribute name="HEIGHT" value="13.49mm"/>
<attribute name="LENGTH" value="11.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003110B"/>
<attribute name="SIZE" value="HC49"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="4.9152 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003127B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003127B?ae"/>
<attribute name="FREQUENCY" value="6 MHz"/>
<attribute name="HEIGHT" value="13.49mm"/>
<attribute name="LENGTH" value="11.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003127B"/>
<attribute name="SIZE" value="HC49"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="6 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003134B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003134B?ae"/>
<attribute name="FREQUENCY" value="6.144 MHz"/>
<attribute name="HEIGHT" value="13.49mm"/>
<attribute name="LENGTH" value="11.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003134B"/>
<attribute name="SIZE" value="HC49"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="6.144 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003147B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003147B?ae"/>
<attribute name="FREQUENCY" value="8 MHz"/>
<attribute name="HEIGHT" value="13.49mm"/>
<attribute name="LENGTH" value="11.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003147B"/>
<attribute name="SIZE" value="HC49"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="8 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003164B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003164B?ae"/>
<attribute name="FREQUENCY" value="10 MHz"/>
<attribute name="HEIGHT" value="13.49mm"/>
<attribute name="LENGTH" value="11.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003164B"/>
<attribute name="SIZE" value="HC49"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="10 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003174B">
<attribute name="C-LOAD" value="pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003174B?ae"/>
<attribute name="FREQUENCY" value="18.432 MHz"/>
<attribute name="HEIGHT" value="13.49mm"/>
<attribute name="LENGTH" value="11.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003174B"/>
<attribute name="SIZE" value="HC49"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="18.432 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003177B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003177B?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="13.49mm"/>
<attribute name="LENGTH" value="11.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003177B"/>
<attribute name="SIZE" value="HC49"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003179B">
<attribute name="C-LOAD" value="pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003179B?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="13.49mm"/>
<attribute name="LENGTH" value="11.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003179B"/>
<attribute name="SIZE" value="HC49"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003206B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003206B?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="13.49mm"/>
<attribute name="LENGTH" value="11.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003206B"/>
<attribute name="SIZE" value="HC49"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003218B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003218B?ae"/>
<attribute name="FREQUENCY" value="14.7456 MHz"/>
<attribute name="HEIGHT" value="13.49mm"/>
<attribute name="LENGTH" value="11.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003218B"/>
<attribute name="SIZE" value="HC49"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="14.7456 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003231B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003231B?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="13.49mm"/>
<attribute name="LENGTH" value="11.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003231B"/>
<attribute name="SIZE" value="HC49"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003257B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003257B?ae"/>
<attribute name="FREQUENCY" value="3.6864 MHz"/>
<attribute name="HEIGHT" value="13.49mm"/>
<attribute name="LENGTH" value="11.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003257B"/>
<attribute name="SIZE" value="HC49"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="3.6864 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003277B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003277B?ae"/>
<attribute name="FREQUENCY" value="9.8304 MHz"/>
<attribute name="HEIGHT" value="13.49mm"/>
<attribute name="LENGTH" value="11.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003277B"/>
<attribute name="SIZE" value="HC49"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="9.8304 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003298B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003298B?ae"/>
<attribute name="FREQUENCY" value="17.73447 MHz"/>
<attribute name="HEIGHT" value="13.49mm"/>
<attribute name="LENGTH" value="11.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003298B"/>
<attribute name="SIZE" value="HC49"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="17.73447 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003312B">
<attribute name="C-LOAD" value="pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003312B?ae"/>
<attribute name="FREQUENCY" value="22.1184 MHz"/>
<attribute name="HEIGHT" value="13.49mm"/>
<attribute name="LENGTH" value="11.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003312B"/>
<attribute name="SIZE" value="HC49"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="22.1184 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003327B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003327B?ae"/>
<attribute name="FREQUENCY" value="11 MHz"/>
<attribute name="HEIGHT" value="13.49mm"/>
<attribute name="LENGTH" value="11.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003327B"/>
<attribute name="SIZE" value="HC49"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="11 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003329B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003329B?ae"/>
<attribute name="FREQUENCY" value="7.3728 MHz"/>
<attribute name="HEIGHT" value="13.49mm"/>
<attribute name="LENGTH" value="11.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003329B"/>
<attribute name="SIZE" value="HC49"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="7.3728 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003342B">
<attribute name="C-LOAD" value="pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003342B?ae"/>
<attribute name="FREQUENCY" value="30 MHz"/>
<attribute name="HEIGHT" value="13.49mm"/>
<attribute name="LENGTH" value="11.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003342B"/>
<attribute name="SIZE" value="HC49"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="30 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003386B">
<attribute name="C-LOAD" value="30pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003386B?ae"/>
<attribute name="FREQUENCY" value="24.576 MHz"/>
<attribute name="HEIGHT" value="13.49mm"/>
<attribute name="LENGTH" value="11.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003386B"/>
<attribute name="SIZE" value="HC49"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="24.576 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
<technology name="_830003515B">
<attribute name="C-LOAD" value="20pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003515B?ae"/>
<attribute name="FREQUENCY" value="11.0592 MHz"/>
<attribute name="HEIGHT" value="13.49mm"/>
<attribute name="LENGTH" value="11.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830003515B"/>
<attribute name="SIZE" value="HC49"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="11.0592 MHz"/>
<attribute name="WIDTH" value="4.7mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XTAL_CFPX-218" prefix="Y">
<description>&lt;b&gt;WE-XTAL Quartz Crystal
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;SMT and THT models
&lt;br&gt; Hermetically sealed
&lt;br&gt; Frequencies between 1.8432 MHz and 50 MHz
&lt;br&gt; Tolerances down to ±10 ppm available
&lt;br&gt; Maximum operating temperatures range: -40 °C to 85 °C
&lt;br&gt; Stabilities down to ±10 ppm available
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;&lt;br&gt;
&lt;br&gt; Microprocessor
&lt;br&gt; Wireless Communication Devices
&lt;br&gt; Industrial Devices
&lt;br&gt; Wired Communication (e.g. Ethernet and USB)
&lt;br&gt; IoT
&lt;br&gt; Optical Network
&lt;br&gt; Audio and Multimedia Devices
&lt;br&gt; Test and Measurement Equipment
&lt;br&gt; Navigation and Locators
&lt;br&gt; Wearables
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135919v209%20WE%20XTAL%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135919v209%20WE%20XTAL%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XTAL&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-10&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CRYSTAL-4PIN"/>
</gates>
<devices>
<device name="" package="WE-XTAL_CFPX-218">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="GND" pad="2" route="any"/>
<connect gate="G$1" pin="GND1" pad="4"/>
</connects>
<technologies>
<technology name="_830050991">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830050991?ae"/>
<attribute name="FREQUENCY" value="26 MHz"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830050991"/>
<attribute name="SIZE" value="CFPX-218"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="26 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830063334">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830063334?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830063334"/>
<attribute name="SIZE" value="CFPX-218"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830069381">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830069381?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830069381"/>
<attribute name="SIZE" value="CFPX-218"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830069383">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830069383?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830069383"/>
<attribute name="SIZE" value="CFPX-218"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830069387">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830069387?ae"/>
<attribute name="FREQUENCY" value="24.576 MHz"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830069387"/>
<attribute name="SIZE" value="CFPX-218"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="24.576 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830069390">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830069390?ae"/>
<attribute name="FREQUENCY" value="32 MHz"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830069390"/>
<attribute name="SIZE" value="CFPX-218"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="32 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830069392">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830069392?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830069392"/>
<attribute name="SIZE" value="CFPX-218"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830069395">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830069395?ae"/>
<attribute name="FREQUENCY" value="16.384 MHz"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830069395"/>
<attribute name="SIZE" value="CFPX-218"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="16.384 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830069400">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830069400?ae"/>
<attribute name="FREQUENCY" value="18.432 MHz"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830069400"/>
<attribute name="SIZE" value="CFPX-218"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="18.432 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830069404">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830069404?ae"/>
<attribute name="FREQUENCY" value="19.2 MHz"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830069404"/>
<attribute name="SIZE" value="CFPX-218"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="19.2 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830069405">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830069405?ae"/>
<attribute name="FREQUENCY" value="27 MHz"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830069405"/>
<attribute name="SIZE" value="CFPX-218"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="27 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830069407">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830069407?ae"/>
<attribute name="FREQUENCY" value="30 MHz"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830069407"/>
<attribute name="SIZE" value="CFPX-218"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="30 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830107284409">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830107284409?ae"/>
<attribute name="FREQUENCY" value="30 MHz"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830107284409"/>
<attribute name="SIZE" value="CFPX-218"/>
<attribute name="STABILITY" value="10ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="30 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830107820709">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830107820709?ae"/>
<attribute name="FREQUENCY" value="32 MHz"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830107820709"/>
<attribute name="SIZE" value="CFPX-218"/>
<attribute name="STABILITY" value="10ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="32 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830107871909">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830107871909?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830107871909"/>
<attribute name="SIZE" value="CFPX-218"/>
<attribute name="STABILITY" value="10ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830108186509">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108186509?ae"/>
<attribute name="FREQUENCY" value="26 MHz"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830108186509"/>
<attribute name="SIZE" value="CFPX-218"/>
<attribute name="STABILITY" value="10ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="26 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830108208009">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108208009?ae"/>
<attribute name="FREQUENCY" value="19.2 MHz"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830108208009"/>
<attribute name="SIZE" value="CFPX-218"/>
<attribute name="STABILITY" value="10ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="19.2 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830108208109">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108208109?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830108208109"/>
<attribute name="SIZE" value="CFPX-218"/>
<attribute name="STABILITY" value="10ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830108208209">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108208209?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830108208209"/>
<attribute name="SIZE" value="CFPX-218"/>
<attribute name="STABILITY" value="10ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830108208409">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108208409?ae"/>
<attribute name="FREQUENCY" value="27 MHz"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830108208409"/>
<attribute name="SIZE" value="CFPX-218"/>
<attribute name="STABILITY" value="10ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="27 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830108208709">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108208709?ae"/>
<attribute name="FREQUENCY" value="40 MHz"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830108208709"/>
<attribute name="SIZE" value="CFPX-218"/>
<attribute name="STABILITY" value="10ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="40 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830108208809">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108208809?ae"/>
<attribute name="FREQUENCY" value="50 MHz"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830108208809"/>
<attribute name="SIZE" value="CFPX-218"/>
<attribute name="STABILITY" value="10ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="50 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XTAL_WATCH" prefix="Y">
<description>&lt;b&gt;WE-XTAL Watch Crystals
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;SMT and THT models
&lt;br&gt;Hermetically sealed
&lt;br&gt;Frequency: 32.768 kHz
&lt;br&gt;Tolerances down to ±10 ppm available
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Microprocessor
&lt;br&gt;Real Time Clocks
&lt;br&gt;Test and Measurement Equipment
&lt;br&gt;Battery powered Applications
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o162740v209%20WE%20Watch%20XTAL%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o162740v209%20WE%20Watch%20XTAL%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XTAL_WATCHCRYSTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XTAL_WATCHCRYSTAL&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CRYSTAL"/>
</gates>
<devices>
<device name="_2X6" package="WE-XTAL_WATCH-2X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_830002997B">
<attribute name="C-LOAD" value="12.5pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830002997B?ae"/>
<attribute name="DIAMETER" value="2mm"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="6.2mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830002997B"/>
<attribute name="SIZE" value="WATCH"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="32.768 kHz"/>
</technology>
<technology name="_830014219B">
<attribute name="C-LOAD" value="6pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830014219B?ae"/>
<attribute name="DIAMETER" value="2mm"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="6.2mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830014219B"/>
<attribute name="SIZE" value="WATCH"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="32.768 kHz"/>
</technology>
</technologies>
</device>
<device name="_3X8" package="WE-XTAL_WATCH-3X8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_830002995B">
<attribute name="C-LOAD" value="12.5pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830002995B?ae"/>
<attribute name="DIAMETER" value="3mm"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="8.2mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830002995B"/>
<attribute name="SIZE" value="WATCH"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="32.768 kHz"/>
</technology>
<technology name="_830002996B">
<attribute name="C-LOAD" value="12.5pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830002996B?ae"/>
<attribute name="DIAMETER" value="3mm"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="8.2mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830002996B"/>
<attribute name="SIZE" value="WATCH"/>
<attribute name="TOLERANCE" value="±15ppm"/>
<attribute name="VALUE" value="32.768 kHz"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XTAL_IQXC-42" prefix="Y">
<description>&lt;b&gt;WE-XTAL Quartz Crystal
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;SMT and THT models
&lt;br&gt; Hermetically sealed
&lt;br&gt; Frequencies between 1.8432 MHz and 50 MHz
&lt;br&gt; Tolerances down to ±10 ppm available
&lt;br&gt; Maximum operating temperatures range: -40 °C to 85 °C
&lt;br&gt; Stabilities down to ±10 ppm available
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;&lt;br&gt;
&lt;br&gt; Microprocessor
&lt;br&gt; Wireless Communication Devices
&lt;br&gt; Industrial Devices
&lt;br&gt; Wired Communication (e.g. Ethernet and USB)
&lt;br&gt; IoT
&lt;br&gt; Optical Network
&lt;br&gt; Audio and Multimedia Devices
&lt;br&gt; Test and Measurement Equipment
&lt;br&gt; Navigation and Locators
&lt;br&gt; Wearables
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135919v209%20WE%20XTAL%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135919v209%20WE%20XTAL%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XTAL&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-10&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CRYSTAL-4PIN"/>
</gates>
<devices>
<device name="" package="WE-XTAL_IQXC-42">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="GND" pad="2" route="any"/>
<connect gate="G$1" pin="GND1" pad="4"/>
</connects>
<technologies>
<technology name="_830059585">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830059585?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830059585"/>
<attribute name="SIZE" value="IQXC-42"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±15ppm"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830059591">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830059591?ae"/>
<attribute name="FREQUENCY" value="26 MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830059591"/>
<attribute name="SIZE" value="IQXC-42"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±15ppm"/>
<attribute name="VALUE" value="26 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830059596">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830059596?ae"/>
<attribute name="FREQUENCY" value="30 MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830059596"/>
<attribute name="SIZE" value="IQXC-42"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±15ppm"/>
<attribute name="VALUE" value="30 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830059597">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830059597?ae"/>
<attribute name="FREQUENCY" value="32 MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830059597"/>
<attribute name="SIZE" value="IQXC-42"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±15ppm"/>
<attribute name="VALUE" value="32 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830059627">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830059627?ae"/>
<attribute name="FREQUENCY" value="38.4 MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830059627"/>
<attribute name="SIZE" value="IQXC-42"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±15ppm"/>
<attribute name="VALUE" value="38.4 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830059632">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830059632?ae"/>
<attribute name="FREQUENCY" value="40 MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830059632"/>
<attribute name="SIZE" value="IQXC-42"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±15ppm"/>
<attribute name="VALUE" value="40 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830069493">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830069493?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830069493"/>
<attribute name="SIZE" value="IQXC-42"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±15ppm"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830069494">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830069494?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830069494"/>
<attribute name="SIZE" value="IQXC-42"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±15ppm"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830072543">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830072543?ae"/>
<attribute name="FREQUENCY" value="27 MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830072543"/>
<attribute name="SIZE" value="IQXC-42"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±15ppm"/>
<attribute name="VALUE" value="27 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830072546">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830072546?ae"/>
<attribute name="FREQUENCY" value="48 MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830072546"/>
<attribute name="SIZE" value="IQXC-42"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±15ppm"/>
<attribute name="VALUE" value="48 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830108178109">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108178109?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108178109"/>
<attribute name="SIZE" value="IQXC-42"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830108212309">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108212309?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108212309"/>
<attribute name="SIZE" value="IQXC-42"/>
<attribute name="STABILITY" value="15ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830108212509">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108212509?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108212509"/>
<attribute name="SIZE" value="IQXC-42"/>
<attribute name="STABILITY" value="15ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830108212609">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108212609?ae"/>
<attribute name="FREQUENCY" value="26 MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108212609"/>
<attribute name="SIZE" value="IQXC-42"/>
<attribute name="STABILITY" value="15ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="26 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830108212709">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108212709?ae"/>
<attribute name="FREQUENCY" value="27.12 MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108212709"/>
<attribute name="SIZE" value="IQXC-42"/>
<attribute name="STABILITY" value="15ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="27.12 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830108212809">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108212809?ae"/>
<attribute name="FREQUENCY" value="30 MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108212809"/>
<attribute name="SIZE" value="IQXC-42"/>
<attribute name="STABILITY" value="15ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="30 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830108212909">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108212909?ae"/>
<attribute name="FREQUENCY" value="32 MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108212909"/>
<attribute name="SIZE" value="IQXC-42"/>
<attribute name="STABILITY" value="15ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="32 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830108213009">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108213009?ae"/>
<attribute name="FREQUENCY" value="37.4 MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108213009"/>
<attribute name="SIZE" value="IQXC-42"/>
<attribute name="STABILITY" value="15ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="37.4 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830108213109">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108213109?ae"/>
<attribute name="FREQUENCY" value="38.4 MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108213109"/>
<attribute name="SIZE" value="IQXC-42"/>
<attribute name="STABILITY" value="15ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="38.4 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830108213209">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108213209?ae"/>
<attribute name="FREQUENCY" value="40 MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108213209"/>
<attribute name="SIZE" value="IQXC-42"/>
<attribute name="STABILITY" value="15ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="40 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830108213509">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108213509?ae"/>
<attribute name="FREQUENCY" value="48 MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108213509"/>
<attribute name="SIZE" value="IQXC-42"/>
<attribute name="STABILITY" value="15ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="48 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830108246809">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108246809?ae"/>
<attribute name="FREQUENCY" value="38.4 MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108246809"/>
<attribute name="SIZE" value="IQXC-42"/>
<attribute name="STABILITY" value="15ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="38.4 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830108288709">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108288709?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="830108288709"/>
<attribute name="SIZE" value="IQXC-42"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XTAL_IQXC-90" prefix="Y">
<description>&lt;b&gt;WE-XTAL Watch Crystals
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;SMT and THT models
&lt;br&gt;Hermetically sealed
&lt;br&gt;Frequency: 32.768 kHz
&lt;br&gt;Tolerances down to ±10 ppm available
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Microprocessor
&lt;br&gt;Real Time Clocks
&lt;br&gt;Test and Measurement Equipment
&lt;br&gt;Battery powered Applications
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o162740v209%20WE%20Watch%20XTAL%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o162740v209%20WE%20Watch%20XTAL%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XTAL_WATCHCRYSTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XTAL_WATCHCRYSTAL&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CRYSTAL"/>
</gates>
<devices>
<device name="" package="WE-XTAL_IQXC-90">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_830065253">
<attribute name="C-LOAD" value="12.5pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830065253?ae"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830065253"/>
<attribute name="SIZE" value="IQXC-90"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="32.768 kHz"/>
<attribute name="WIDTH" value="1mm"/>
</technology>
<technology name="_830066198">
<attribute name="C-LOAD" value="9pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830066198?ae"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830066198"/>
<attribute name="SIZE" value="IQXC-90"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="32.768 kHz"/>
<attribute name="WIDTH" value="1mm"/>
</technology>
<technology name="_830066431">
<attribute name="C-LOAD" value="7pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830066431?ae"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830066431"/>
<attribute name="SIZE" value="IQXC-90"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="32.768 kHz"/>
<attribute name="WIDTH" value="1mm"/>
</technology>
<technology name="_830107088501">
<attribute name="C-LOAD" value="6pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830107088501?ae"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830107088501"/>
<attribute name="SIZE" value="IQXC-90"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="32.768 kHz"/>
<attribute name="WIDTH" value="1mm"/>
</technology>
<technology name="_830108214001">
<attribute name="C-LOAD" value="4pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108214001?ae"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108214001"/>
<attribute name="SIZE" value="IQXC-90"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="32.768 kHz"/>
<attribute name="WIDTH" value="1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XTAL_IQXC-240" prefix="Y">
<description>&lt;b&gt;WE-XTAL Quartz Crystal
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;SMT and THT models
&lt;br&gt; Hermetically sealed
&lt;br&gt; Frequencies between 1.8432 MHz and 50 MHz
&lt;br&gt; Tolerances down to ±10 ppm available
&lt;br&gt; Maximum operating temperatures range: -40 °C to 85 °C
&lt;br&gt; Stabilities down to ±10 ppm available
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;&lt;br&gt;
&lt;br&gt; Microprocessor
&lt;br&gt; Wireless Communication Devices
&lt;br&gt; Industrial Devices
&lt;br&gt; Wired Communication (e.g. Ethernet and USB)
&lt;br&gt; IoT
&lt;br&gt; Optical Network
&lt;br&gt; Audio and Multimedia Devices
&lt;br&gt; Test and Measurement Equipment
&lt;br&gt; Navigation and Locators
&lt;br&gt; Wearables
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135919v209%20WE%20XTAL%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135919v209%20WE%20XTAL%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XTAL&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-10&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CRYSTAL-4PIN_NC"/>
</gates>
<devices>
<device name="" package="WE-XTAL_IQXC-240">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="N/C" pad="4"/>
</connects>
<technologies>
<technology name="_830108049101">
<attribute name="C-LOAD" value="8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108049101?ae"/>
<attribute name="FREQUENCY" value="48 MHz"/>
<attribute name="HEIGHT" value="0.33mm"/>
<attribute name="LENGTH" value="1.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-30 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108049101"/>
<attribute name="SIZE" value="IQXC-240"/>
<attribute name="STABILITY" value="10ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="48 MHz"/>
<attribute name="WIDTH" value="1mm"/>
</technology>
<technology name="_830108131401">
<attribute name="C-LOAD" value="5pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108131401?ae"/>
<attribute name="FREQUENCY" value="37.4 MHz"/>
<attribute name="HEIGHT" value="0.33mm"/>
<attribute name="LENGTH" value="1.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-30 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108131401"/>
<attribute name="SIZE" value="IQXC-240"/>
<attribute name="STABILITY" value="15ppm"/>
<attribute name="TOLERANCE" value="±7ppm"/>
<attribute name="VALUE" value="37.4 MHz"/>
<attribute name="WIDTH" value="1mm"/>
</technology>
<technology name="_830108131601">
<attribute name="C-LOAD" value="5pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108131601?ae"/>
<attribute name="FREQUENCY" value="38.4 MHz"/>
<attribute name="HEIGHT" value="0.33mm"/>
<attribute name="LENGTH" value="1.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-30 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108131601"/>
<attribute name="SIZE" value="IQXC-240"/>
<attribute name="STABILITY" value="15ppm"/>
<attribute name="TOLERANCE" value="±7ppm"/>
<attribute name="VALUE" value="38.4 MHz"/>
<attribute name="WIDTH" value="1mm"/>
</technology>
<technology name="_830108254201">
<attribute name="C-LOAD" value="5pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830108254201?ae"/>
<attribute name="FREQUENCY" value="32 MHz"/>
<attribute name="HEIGHT" value="0.33mm"/>
<attribute name="LENGTH" value="1.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-30 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830108254201"/>
<attribute name="SIZE" value="IQXC-240"/>
<attribute name="STABILITY" value="15ppm"/>
<attribute name="TOLERANCE" value="±7ppm"/>
<attribute name="VALUE" value="32 MHz"/>
<attribute name="WIDTH" value="1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XTAL_CFPX-104" prefix="Y">
<description>&lt;b&gt;WE-XTAL Quartz Crystal
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;SMT and THT models
&lt;br&gt; Hermetically sealed
&lt;br&gt; Frequencies between 1.8432 MHz and 50 MHz
&lt;br&gt; Tolerances down to ±10 ppm available
&lt;br&gt; Maximum operating temperatures range: -40 °C to 85 °C
&lt;br&gt; Stabilities down to ±10 ppm available
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;&lt;br&gt;
&lt;br&gt; Microprocessor
&lt;br&gt; Wireless Communication Devices
&lt;br&gt; Industrial Devices
&lt;br&gt; Wired Communication (e.g. Ethernet and USB)
&lt;br&gt; IoT
&lt;br&gt; Optical Network
&lt;br&gt; Audio and Multimedia Devices
&lt;br&gt; Test and Measurement Equipment
&lt;br&gt; Navigation and Locators
&lt;br&gt; Wearables
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135919v209%20WE%20XTAL%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135919v209%20WE%20XTAL%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XTAL&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-10&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CRYSTAL-4PIN"/>
</gates>
<devices>
<device name="" package="WE-XTAL_CFPX-104">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND1" pad="4"/>
</connects>
<technologies>
<technology name="_830030819">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830030819?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830030819"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±50ppm"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830030820">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830030820?ae"/>
<attribute name="FREQUENCY" value="30 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830030820"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±50ppm"/>
<attribute name="VALUE" value="30 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830032817">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830032817?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830032817"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±50ppm"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830032878">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830032878?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830032878"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±50ppm"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830033075">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830033075?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830033075"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±50ppm"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830033328">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830033328?ae"/>
<attribute name="FREQUENCY" value="14.7456 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830033328"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±50ppm"/>
<attribute name="VALUE" value="14.7456 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830033643">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830033643?ae"/>
<attribute name="FREQUENCY" value="14.31818 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830033643"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±50ppm"/>
<attribute name="VALUE" value="14.31818 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830033644">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830033644?ae"/>
<attribute name="FREQUENCY" value="24.576 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830033644"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±50ppm"/>
<attribute name="VALUE" value="24.576 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830033645">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830033645?ae"/>
<attribute name="FREQUENCY" value="40 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-10 °C up to +60 °C"/>
<attribute name="PART-NUMBER" value="830033645"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±50ppm"/>
<attribute name="VALUE" value="40 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830036401">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830036401?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830036401"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830053798">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830053798?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830053798"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830055663">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830055663?ae"/>
<attribute name="FREQUENCY" value="8 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830055663"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="8 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830055901">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830055901?ae"/>
<attribute name="FREQUENCY" value="8 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830055901"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="8 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830055999">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830055999?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830055999"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830056556">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830056556?ae"/>
<attribute name="FREQUENCY" value="12.5 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830056556"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±50ppm"/>
<attribute name="VALUE" value="12.5 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830056583">
<attribute name="C-LOAD" value="12pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830056583?ae"/>
<attribute name="FREQUENCY" value="10 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830056583"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="10 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830056808">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830056808?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830056808"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830059477">
<attribute name="C-LOAD" value="15pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830059477?ae"/>
<attribute name="FREQUENCY" value="12.8 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830059477"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="12.8 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830059522">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830059522?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830059522"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830059523">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830059523?ae"/>
<attribute name="FREQUENCY" value="12.288 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830059523"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="12.288 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830059526">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830059526?ae"/>
<attribute name="FREQUENCY" value="14.31818 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830059526"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="14.31818 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830059528">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830059528?ae"/>
<attribute name="FREQUENCY" value="16.384 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830059528"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="16.384 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830059529">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830059529?ae"/>
<attribute name="FREQUENCY" value="18.432 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830059529"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="18.432 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830059530">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830059530?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830059530"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830059531">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830059531?ae"/>
<attribute name="FREQUENCY" value="24.576 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830059531"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="24.576 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830059532">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830059532?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830059532"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830059535">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830059535?ae"/>
<attribute name="FREQUENCY" value="32 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830059535"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="32 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830059537">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830059537?ae"/>
<attribute name="FREQUENCY" value="40 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830059537"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="40 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830059539">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830059539?ae"/>
<attribute name="FREQUENCY" value="48 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830059539"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="48 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830061486">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830061486?ae"/>
<attribute name="FREQUENCY" value="8.192 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830061486"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="8.192 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830065460">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830065460?ae"/>
<attribute name="FREQUENCY" value="30 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830065460"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="20ppm"/>
<attribute name="TOLERANCE" value="±10ppm"/>
<attribute name="VALUE" value="30 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830072402">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830072402?ae"/>
<attribute name="FREQUENCY" value="10 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830072402"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="10 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830072403">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830072403?ae"/>
<attribute name="FREQUENCY" value="14.7456 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830072403"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="14.7456 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830072404">
<attribute name="C-LOAD" value="18pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830072404?ae"/>
<attribute name="FREQUENCY" value="26 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830072404"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="26 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830106162701">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830106162701?ae"/>
<attribute name="FREQUENCY" value="8 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830106162701"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="8 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_830106163301">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830106163301?ae"/>
<attribute name="FREQUENCY" value="13.56 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830106163301"/>
<attribute name="SIZE" value="CFPX-104"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="13.56 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XTAL_85SMX" prefix="Y">
<description>&lt;b&gt;WE-XTAL Watch Crystals
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;SMT and THT models
&lt;br&gt;Hermetically sealed
&lt;br&gt;Frequency: 32.768 kHz
&lt;br&gt;Tolerances down to ±10 ppm available
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Microprocessor
&lt;br&gt;Real Time Clocks
&lt;br&gt;Test and Measurement Equipment
&lt;br&gt;Battery powered Applications
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o162740v209%20WE%20Watch%20XTAL%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o162740v209%20WE%20Watch%20XTAL%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XTAL_WATCHCRYSTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XTAL_WATCHCRYSTAL&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CRYSTAL-4PIN"/>
</gates>
<devices>
<device name="" package="WE-XTAL_85SMX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="GND" pad="2" route="any"/>
<connect gate="G$1" pin="GND1" pad="3"/>
</connects>
<technologies>
<technology name="_830003000">
<attribute name="C-LOAD" value="12.5pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830003000?ae"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="8.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830003000"/>
<attribute name="SIZE" value="85SMX"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="32.768 kHz"/>
<attribute name="WIDTH" value="3.7mm"/>
</technology>
<technology name="_830016178">
<attribute name="C-LOAD" value="6pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830016178?ae"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="8.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830016178"/>
<attribute name="SIZE" value="85SMX"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="32.768 kHz"/>
<attribute name="WIDTH" value="3.7mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XTAL_CFPX-217" prefix="Y">
<description>&lt;b&gt;WE-XTAL Watch Crystals
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;SMT and THT models
&lt;br&gt;Hermetically sealed
&lt;br&gt;Frequency: 32.768 kHz
&lt;br&gt;Tolerances down to ±10 ppm available
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Microprocessor
&lt;br&gt;Real Time Clocks
&lt;br&gt;Test and Measurement Equipment
&lt;br&gt;Battery powered Applications
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o162740v209%20WE%20Watch%20XTAL%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o162740v209%20WE%20Watch%20XTAL%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XTAL_WATCHCRYSTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XTAL_WATCHCRYSTAL&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CRYSTAL"/>
</gates>
<devices>
<device name="" package="WE-XTAL_CFPX-217">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_830009678">
<attribute name="C-LOAD" value="12.5pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830009678?ae"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="0.9mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830009678"/>
<attribute name="SIZE" value="CFPX-217"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="32.768 kHz"/>
<attribute name="WIDTH" value="1.5mm"/>
</technology>
<technology name="_830009706">
<attribute name="C-LOAD" value="9pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830009706?ae"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="0.9mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830009706"/>
<attribute name="SIZE" value="CFPX-217"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="32.768 kHz"/>
<attribute name="WIDTH" value="1.5mm"/>
</technology>
<technology name="_830009709">
<attribute name="C-LOAD" value="7pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830009709?ae"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="0.9mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830009709"/>
<attribute name="SIZE" value="CFPX-217"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="32.768 kHz"/>
<attribute name="WIDTH" value="1.5mm"/>
</technology>
<technology name="_830054236">
<attribute name="C-LOAD" value="6pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830054236?ae"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="0.9mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="830054236"/>
<attribute name="SIZE" value="CFPX-217"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="32.768 kHz"/>
<attribute name="WIDTH" value="1.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XTAL_12SMX" prefix="Y">
<description>&lt;b&gt;WE-XTAL Quartz Crystal
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;SMT and THT models
&lt;br&gt; Hermetically sealed
&lt;br&gt; Frequencies between 1.8432 MHz and 50 MHz
&lt;br&gt; Tolerances down to ±10 ppm available
&lt;br&gt; Maximum operating temperatures range: -40 °C to 85 °C
&lt;br&gt; Stabilities down to ±10 ppm available
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;&lt;br&gt;
&lt;br&gt; Microprocessor
&lt;br&gt; Wireless Communication Devices
&lt;br&gt; Industrial Devices
&lt;br&gt; Wired Communication (e.g. Ethernet and USB)
&lt;br&gt; IoT
&lt;br&gt; Optical Network
&lt;br&gt; Audio and Multimedia Devices
&lt;br&gt; Test and Measurement Equipment
&lt;br&gt; Navigation and Locators
&lt;br&gt; Wearables
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135919v209%20WE%20XTAL%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135919v209%20WE%20XTAL%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XTAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XTAL&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-10&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CRYSTAL-4PIN"/>
</gates>
<devices>
<device name="" package="WE-XTAL_12SMX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND1" pad="4"/>
</connects>
<technologies>
<technology name="_830026380">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830026380?ae"/>
<attribute name="FREQUENCY" value="8 MHz"/>
<attribute name="HEIGHT" value="1.4mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830026380"/>
<attribute name="SIZE" value="12SMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="8 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_830026382">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830026382?ae"/>
<attribute name="FREQUENCY" value="11.0592 MHz"/>
<attribute name="HEIGHT" value="1.4mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830026382"/>
<attribute name="SIZE" value="12SMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="11.0592 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_830026384">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830026384?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="1.4mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830026384"/>
<attribute name="SIZE" value="12SMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_830026386">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830026386?ae"/>
<attribute name="FREQUENCY" value="14.31818 MHz"/>
<attribute name="HEIGHT" value="1.4mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830026386"/>
<attribute name="SIZE" value="12SMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="14.31818 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_830026388">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830026388?ae"/>
<attribute name="FREQUENCY" value="14.7456 MHz"/>
<attribute name="HEIGHT" value="1.4mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830026388"/>
<attribute name="SIZE" value="12SMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="14.7456 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_830026392">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830026392?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="1.4mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830026392"/>
<attribute name="SIZE" value="12SMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_830026394">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830026394?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="1.4mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830026394"/>
<attribute name="SIZE" value="12SMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_830026396">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830026396?ae"/>
<attribute name="FREQUENCY" value="24.576 MHz"/>
<attribute name="HEIGHT" value="1.4mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830026396"/>
<attribute name="SIZE" value="12SMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="24.576 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_830026504">
<attribute name="C-LOAD" value="16pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830026504?ae"/>
<attribute name="FREQUENCY" value="30 MHz"/>
<attribute name="HEIGHT" value="1.4mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830026504"/>
<attribute name="SIZE" value="12SMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±30ppm"/>
<attribute name="VALUE" value="30 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_830059082">
<attribute name="C-LOAD" value="10pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830059082?ae"/>
<attribute name="FREQUENCY" value="8 MHz"/>
<attribute name="HEIGHT" value="1.4mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="830059082"/>
<attribute name="SIZE" value="12SMX"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="TOLERANCE" value="±20ppm"/>
<attribute name="VALUE" value="8 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>